****************************************************************************

		  ADMtek ADM8511 USB To Fast Ethernet Adapter

			     Release Information
			     ~~~~~~~~~~~~~~~~~~~

		   Copyright (C) 1999 ADMtek Incorporated.
			     All rights reserved.

				   V2.05		       Mar. 15, 2001
****************************************************************************

  Welcome to Fast Ethernet Controller Provider's growing family of users,
and thank you for purchasing one of our networking products.


Diskette Contents
=================

Files and
Subdirectories		Description
----------------------------------------------------------------------------
ADM8511.SYS		The NDIS 5 driver support Windows 98/98_SE/ME, 
			windows 2000 on x86 platform.

NET8511.CAT		Security catalog.

NET8511.INF		The NDIS 5 driver installation information file.

AN986N.INF		The NDIS 5 driver installation information file.

RELEASE.TXT		This file presents a summary of the contents of your
			Driver Diskette and record of revisions for driver
			releases.

----------------------------------------------------------------------------


Driver/Utility Version
======================

Driver/Utility					Filename	Version
----------------------------------------------------------------------------

NDIS 5 Driver(Windows 98/98_SE, windows 2000)	ADM8511.SYS	2.05

----------------------------------------------------------------------------


RECORD OF REVISIONS FOR DRIVER RELEASES
=======================================

Release Number / Date		Changes
----------------------------------------------------------------------------
  V2.00		08/21/2000	Supported BOTH AMD & NS homephy, and 
				supported NS C version.
----------------------------------------------------------------------------
  V2.01		09/14/2000	1.Supported AD version.(not supported AC 
				  version)
				2.Fixed Autosense cannot change from HomePNA
				  to Ethernet.
				3.Remove all "ADMtek" this word.
				4.Test mode change default value. Form
				  Mode1->Mode2.(modified .inf file)
----------------------------------------------------------------------------
 V2.02		09/25/2000	Use GPIO3 to indicate Link Status.Supported 
				NS HomePNA phyter C version test mode.(NS 
				chip pin 43 must tie to ground).(we did need
				reset PHY in check for hang routine.)
----------------------------------------------------------------------------
 V2.03		11/20/2000	Just adjust source code.
----------------------------------------------------------------------------
 V2.04		02/09/2001	For pass whislter submission.(add free 
				ndispacket & ndisbuffer).Add performance 
				improving function(add 3 LM_Qreceivepacket 
				before leaving LM_Reset adapter).
				PS. This version only have ADMtek brand.
----------------------------------------------------------------------------
 V2.05		03/15/2001	Some indicate Link status different with
				v2.04.
----------------------------------------------------------------------------
--- End of File ---

 *** All trademarks or brand names mentioned are trademarks or registered
 *** trademarks of their respective companies.

