MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=2
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=2.000
fDecay=0.900
fVideoEchoZoom=1.007
fVideoEchoAlpha=0.500
nVideoEchoOrientation=1
nWaveMode=1
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=1
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=1
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=1.000
fWaveSmoothing=0.750
fWaveParam=0.000
fModWaveAlphaStart=0.750
fModWaveAlphaEnd=0.950
fWarpAnimSpeed=1.000
fWarpScale=1.000
fZoomExponent=1.00000
fShader=0.000
zoom=0.96000
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.00052
sx=1.00000
sy=1.00000
wave_r=0.000
wave_g=0.000
wave_b=0.000
wave_x=0.500
wave_y=0.500
ob_size=0.010
ob_r=1.000
ob_g=1.000
ob_b=1.000
ob_a=0.000
ib_size=0.010
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.900
mv_r=1.000
mv_g=1.000
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=1
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=1
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_per_point1=//apply zoom burst on beat
wave_0_per_point2=flag = above(q3,2);
wave_0_per_point3=//state zero is ready state
wave_0_per_point4=state = state + flag*equal(state,0);
wave_0_per_point5=
wave_0_per_point6=//upwards flight
wave_0_per_point7=yval = if(equal(state,0),0, yval);
wave_0_per_point8=yval = yval + 0.00004*equal(state,1);
wave_0_per_point9=ymax = if(equal(state,0),rand(100)*0.004,ymax);
wave_0_per_point10=
wave_0_per_point11=//hit apogee
wave_0_per_point12=state = if(above(yval,0.5+ymax),2,state);
wave_0_per_point13=
wave_0_per_point14=//reset variable
wave_0_per_point15=yval = if(equal(state,0),0, yval);
wave_0_per_point16=burst = if(equal(state,0),0.001,burst);
wave_0_per_point17=alphax = if(equal(state,0),1,alphax);
wave_0_per_point18=xdriftinc = if(equal(state,0),0,xdriftinc);
wave_0_per_point19=
wave_0_per_point20=burstspeed = if(equal(state,0),rand(10),burstspeed);
wave_0_per_point21=xdrift = if(equal(state,0),rand(20),xdrift);
wave_0_per_point22=//to get the numbers small enough have to use constants
wave_0_per_point23=xdriftinc = xdriftinc
wave_0_per_point24=+ equal(xdrift,0)*equal(state,1)*0.00002
wave_0_per_point25=+ equal(xdrift,1)*equal(state,1)*0.000018
wave_0_per_point26=+ equal(xdrift,2)*equal(state,1)*0.000016
wave_0_per_point27=+ equal(xdrift,3)*equal(state,1)*0.000014
wave_0_per_point28=+ equal(xdrift,4)*equal(state,1)*0.000012
wave_0_per_point29=+ equal(xdrift,5)*equal(state,1)*0.00001
wave_0_per_point30=+ equal(xdrift,6)*equal(state,1)*0.000008
wave_0_per_point31=+ equal(xdrift,7)*equal(state,1)*0.000006
wave_0_per_point32=+ equal(xdrift,8)*equal(state,1)*0.000004
wave_0_per_point33=+ equal(xdrift,9)*equal(state,1)*0.000002
wave_0_per_point34=+ equal(xdrift,11)*equal(state,1)*-0.000002
wave_0_per_point35=+ equal(xdrift,12)*equal(state,1)*-0.000004
wave_0_per_point36=+ equal(xdrift,13)*equal(state,1)*-0.000006
wave_0_per_point37=+ equal(xdrift,14)*equal(state,1)*-0.000008
wave_0_per_point38=+ equal(xdrift,15)*equal(state,1)*-0.00001
wave_0_per_point39=+ equal(xdrift,16)*equal(state,1)*-0.000012
wave_0_per_point40=+ equal(xdrift,17)*equal(state,1)*-0.000014
wave_0_per_point41=+ equal(xdrift,18)*equal(state,1)*-0.000016
wave_0_per_point42=+ equal(xdrift,19)*equal(state,1)*-0.000018;
wave_0_per_point43=
wave_0_per_point44=burst = burst
wave_0_per_point45=+ equal(burstspeed,0)*equal(state,2)*0.000024
wave_0_per_point46=+ equal(burstspeed,1)*equal(state,2)*0.000022
wave_0_per_point47=+ equal(burstspeed,2)*equal(state,2)*0.00002
wave_0_per_point48=+ equal(burstspeed,3)*equal(state,2)*0.000018
wave_0_per_point49=+ equal(burstspeed,4)*equal(state,2)*0.000016
wave_0_per_point50=+ equal(burstspeed,5)*equal(state,2)*0.000014
wave_0_per_point51=+ equal(burstspeed,6)*equal(state,2)*0.000012
wave_0_per_point52=+ equal(burstspeed,7)*equal(state,2)*0.00001
wave_0_per_point53=+ equal(burstspeed,8)*equal(state,2)*0.000008
wave_0_per_point54=+ equal(burstspeed,9)*equal(state,2)*0.000008;
wave_0_per_point55=
wave_0_per_point56=alphax = alphax - 0.00004*equal(state,2);
wave_0_per_point57=state = if(below(alphax,0),0,state);
wave_0_per_point58=
wave_0_per_point59=
wave_0_per_point60=s = sample*3.14*100;
wave_0_per_point61=ss = sample*6.28*1000;
wave_0_per_point62=
wave_0_per_point63=//draw torus
wave_0_per_point64=xs = (burst*0.1 + burst*cos(s))*cos(ss);
wave_0_per_point65=ys = (burst*0.1 + burst*cos(s))*sin(ss);
wave_0_per_point66=zs = burst*sin(s);
wave_0_per_point67=
wave_0_per_point68=
wave_0_per_point69=//rotate x axis
wave_0_per_point70=angle = sin(q1*0.025)*6.28;
wave_0_per_point71=yx = ys*cos(angle) - zs*sin(angle);
wave_0_per_point72=zx = ys*sin(angle) + zs*cos(angle);
wave_0_per_point73=xx = xs;
wave_0_per_point74=
wave_0_per_point75=//rotate y axis
wave_0_per_point76=angle2 = sin(q1*0.03)*6.28;
wave_0_per_point77=xd = xx*cos(angle2) - zx*sin(angle2);
wave_0_per_point78=zd = xx*sin(angle2) + zx*cos(angle2);
wave_0_per_point79=yd = yx;
wave_0_per_point80=
wave_0_per_point81=//rotaye z axis
wave_0_per_point82=angle3 = sin(q1*0.022)*6.28;
wave_0_per_point83=xn = xd*cos(angle3) - yd*sin(angle3);
wave_0_per_point84=yn = xd*sin(angle3) + yd*cos(angle3);
wave_0_per_point85=
wave_0_per_point86=zd = zd + 2;
wave_0_per_point87=
wave_0_per_point88=x = xn*zd*0.3 + 0.5;
wave_0_per_point89=y = yn*zd*0.3*1.2;
wave_0_per_point90=
wave_0_per_point91=
wave_0_per_point92=x = x + xdriftinc;
wave_0_per_point93=y = y + sin(yval*1.5) - 0.18;
wave_0_per_point94=
wave_0_per_point95=
wave_0_per_point96=r = 0.5 + 0.5*sin(q1*1.2 + x + x);
wave_0_per_point97=g = 0.5 + 0.5*sin(q1*1.5 + x + y);
wave_0_per_point98=b = 0.5 + 0.5*sin(q1*1.36 + y + y);
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=1
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=1
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_point1=//apply zoom burst on beat
wave_1_per_point2=flag = above(q3,2);
wave_1_per_point3=//state zero is ready state
wave_1_per_point4=state = state + flag*equal(state,0);
wave_1_per_point5=
wave_1_per_point6=//upwards flight
wave_1_per_point7=yval = if(equal(state,0),0, yval);
wave_1_per_point8=yval = yval + 0.00004*equal(state,1);
wave_1_per_point9=ymax = if(equal(state,0),rand(100)*0.004,ymax);
wave_1_per_point10=
wave_1_per_point11=//hit apogee
wave_1_per_point12=state = if(above(yval,0.5+ymax),2,state);
wave_1_per_point13=
wave_1_per_point14=//reset variable
wave_1_per_point15=yval = if(equal(state,0),0, yval);
wave_1_per_point16=burst = if(equal(state,0),0.001,burst);
wave_1_per_point17=alphax = if(equal(state,0),1,alphax);
wave_1_per_point18=xdriftinc = if(equal(state,0),0,xdriftinc);
wave_1_per_point19=
wave_1_per_point20=burstspeed = if(equal(state,0),rand(10),burstspeed);
wave_1_per_point21=xdrift = if(equal(state,0),rand(20),xdrift);
wave_1_per_point22=//to get the numbers small enough have to use constants
wave_1_per_point23=xdriftinc = xdriftinc
wave_1_per_point24=+ equal(xdrift,0)*equal(state,1)*0.00002
wave_1_per_point25=+ equal(xdrift,1)*equal(state,1)*0.000018
wave_1_per_point26=+ equal(xdrift,2)*equal(state,1)*0.000016
wave_1_per_point27=+ equal(xdrift,3)*equal(state,1)*0.000014
wave_1_per_point28=+ equal(xdrift,4)*equal(state,1)*0.000012
wave_1_per_point29=+ equal(xdrift,5)*equal(state,1)*0.00001
wave_1_per_point30=+ equal(xdrift,6)*equal(state,1)*0.000008
wave_1_per_point31=+ equal(xdrift,7)*equal(state,1)*0.000006
wave_1_per_point32=+ equal(xdrift,8)*equal(state,1)*0.000004
wave_1_per_point33=+ equal(xdrift,9)*equal(state,1)*0.000002
wave_1_per_point34=+ equal(xdrift,11)*equal(state,1)*-0.000002
wave_1_per_point35=+ equal(xdrift,12)*equal(state,1)*-0.000004
wave_1_per_point36=+ equal(xdrift,13)*equal(state,1)*-0.000006
wave_1_per_point37=+ equal(xdrift,14)*equal(state,1)*-0.000008
wave_1_per_point38=+ equal(xdrift,15)*equal(state,1)*-0.00001
wave_1_per_point39=+ equal(xdrift,16)*equal(state,1)*-0.000012
wave_1_per_point40=+ equal(xdrift,17)*equal(state,1)*-0.000014
wave_1_per_point41=+ equal(xdrift,18)*equal(state,1)*-0.000016
wave_1_per_point42=+ equal(xdrift,19)*equal(state,1)*-0.000018;
wave_1_per_point43=
wave_1_per_point44=burst = burst
wave_1_per_point45=+ equal(burstspeed,0)*equal(state,2)*0.000024
wave_1_per_point46=+ equal(burstspeed,1)*equal(state,2)*0.000022
wave_1_per_point47=+ equal(burstspeed,2)*equal(state,2)*0.00002
wave_1_per_point48=+ equal(burstspeed,3)*equal(state,2)*0.000018
wave_1_per_point49=+ equal(burstspeed,4)*equal(state,2)*0.000016
wave_1_per_point50=+ equal(burstspeed,5)*equal(state,2)*0.000014
wave_1_per_point51=+ equal(burstspeed,6)*equal(state,2)*0.000012
wave_1_per_point52=+ equal(burstspeed,7)*equal(state,2)*0.00001
wave_1_per_point53=+ equal(burstspeed,8)*equal(state,2)*0.000008
wave_1_per_point54=+ equal(burstspeed,9)*equal(state,2)*0.000008;
wave_1_per_point55=
wave_1_per_point56=alphax = alphax - 0.00004*equal(state,2);
wave_1_per_point57=state = if(below(alphax,0),0,state);
wave_1_per_point58=
wave_1_per_point59=
wave_1_per_point60=s = sample*3.14*100;
wave_1_per_point61=ss = sample*6.28*1000;
wave_1_per_point62=
wave_1_per_point63=//draw torus
wave_1_per_point64=xs = (burst + 0.0001*cos(s))*cos(ss);
wave_1_per_point65=ys = (burst + 0.0001*cos(s))*sin(ss);
wave_1_per_point66=zs = 0.1*burst*sin(s);
wave_1_per_point67=
wave_1_per_point68=
wave_1_per_point69=//rotate x axis
wave_1_per_point70=angle = sin(-q1*0.035)*6.28;
wave_1_per_point71=yx = ys*cos(angle) - zs*sin(angle);
wave_1_per_point72=zx = ys*sin(angle) + zs*cos(angle);
wave_1_per_point73=xx = xs;
wave_1_per_point74=
wave_1_per_point75=//rotate y axis
wave_1_per_point76=angle2 = sin(q1*0.03)*6.28;
wave_1_per_point77=xd = xx*cos(angle2) - zx*sin(angle2);
wave_1_per_point78=zd = xx*sin(angle2) + zx*cos(angle2);
wave_1_per_point79=yd = yx;
wave_1_per_point80=
wave_1_per_point81=//rotaye z axis
wave_1_per_point82=angle3 = sin(-q1*0.032)*6.28;
wave_1_per_point83=xn = xd*cos(angle3) - yd*sin(angle3);
wave_1_per_point84=yn = xd*sin(angle3) + yd*cos(angle3);
wave_1_per_point85=
wave_1_per_point86=zd = zd + 2;
wave_1_per_point87=
wave_1_per_point88=x = xn*zd*0.3 + 0.5;
wave_1_per_point89=y = yn*zd*0.3*1.2;
wave_1_per_point90=
wave_1_per_point91=
wave_1_per_point92=x = x + xdriftinc;
wave_1_per_point93=y = y + sin(yval*1.5) - 0.18;
wave_1_per_point94=
wave_1_per_point95=
wave_1_per_point96=r = 0.5 + 0.5*sin(q1*1.7 + x + x);
wave_1_per_point97=g = 0.5 + 0.5*sin(q1*1.5 + x + y);
wave_1_per_point98=b = 0.5 + 0.5*sin(q1*1.16 + y + y);
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=1
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=0
wavecode_2_bAdditive=1
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_point1=//apply zoom burst on beat
wave_2_per_point2=flag = above(q3,2);
wave_2_per_point3=//state zero is ready state
wave_2_per_point4=state = state + flag*equal(state,0);
wave_2_per_point5=
wave_2_per_point6=//upwards flight
wave_2_per_point7=yval = if(equal(state,0),0, yval);
wave_2_per_point8=yval = yval + 0.00004*equal(state,1);
wave_2_per_point9=ymax = if(equal(state,0),rand(100)*0.004,ymax);
wave_2_per_point10=
wave_2_per_point11=//hit apogee
wave_2_per_point12=state = if(above(yval,0.5+ymax),2,state);
wave_2_per_point13=
wave_2_per_point14=//reset variable
wave_2_per_point15=yval = if(equal(state,0),0, yval);
wave_2_per_point16=burst = if(equal(state,0),0.001,burst);
wave_2_per_point17=alphax = if(equal(state,0),1,alphax);
wave_2_per_point18=xdriftinc = if(equal(state,0),0,xdriftinc);
wave_2_per_point19=
wave_2_per_point20=burstspeed = if(equal(state,0),rand(10),burstspeed);
wave_2_per_point21=xdrift = if(equal(state,0),rand(20),xdrift);
wave_2_per_point22=//to get the numbers small enough have to use constants
wave_2_per_point23=xdriftinc = xdriftinc
wave_2_per_point24=+ equal(xdrift,0)*equal(state,1)*0.00002
wave_2_per_point25=+ equal(xdrift,1)*equal(state,1)*0.000018
wave_2_per_point26=+ equal(xdrift,2)*equal(state,1)*0.000016
wave_2_per_point27=+ equal(xdrift,3)*equal(state,1)*0.000014
wave_2_per_point28=+ equal(xdrift,4)*equal(state,1)*0.000012
wave_2_per_point29=+ equal(xdrift,5)*equal(state,1)*0.00001
wave_2_per_point30=+ equal(xdrift,6)*equal(state,1)*0.000008
wave_2_per_point31=+ equal(xdrift,7)*equal(state,1)*0.000006
wave_2_per_point32=+ equal(xdrift,8)*equal(state,1)*0.000004
wave_2_per_point33=+ equal(xdrift,9)*equal(state,1)*0.000002
wave_2_per_point34=+ equal(xdrift,11)*equal(state,1)*-0.000002
wave_2_per_point35=+ equal(xdrift,12)*equal(state,1)*-0.000004
wave_2_per_point36=+ equal(xdrift,13)*equal(state,1)*-0.000006
wave_2_per_point37=+ equal(xdrift,14)*equal(state,1)*-0.000008
wave_2_per_point38=+ equal(xdrift,15)*equal(state,1)*-0.00001
wave_2_per_point39=+ equal(xdrift,16)*equal(state,1)*-0.000012
wave_2_per_point40=+ equal(xdrift,17)*equal(state,1)*-0.000014
wave_2_per_point41=+ equal(xdrift,18)*equal(state,1)*-0.000016
wave_2_per_point42=+ equal(xdrift,19)*equal(state,1)*-0.000018;
wave_2_per_point43=
wave_2_per_point44=burst = burst
wave_2_per_point45=+ equal(burstspeed,0)*equal(state,2)*0.000024
wave_2_per_point46=+ equal(burstspeed,1)*equal(state,2)*0.000022
wave_2_per_point47=+ equal(burstspeed,2)*equal(state,2)*0.00002
wave_2_per_point48=+ equal(burstspeed,3)*equal(state,2)*0.000018
wave_2_per_point49=+ equal(burstspeed,4)*equal(state,2)*0.000016
wave_2_per_point50=+ equal(burstspeed,5)*equal(state,2)*0.000014
wave_2_per_point51=+ equal(burstspeed,6)*equal(state,2)*0.000012
wave_2_per_point52=+ equal(burstspeed,7)*equal(state,2)*0.00001
wave_2_per_point53=+ equal(burstspeed,8)*equal(state,2)*0.000008
wave_2_per_point54=+ equal(burstspeed,9)*equal(state,2)*0.000008;
wave_2_per_point55=
wave_2_per_point56=alphax = alphax - 0.00004*equal(state,2);
wave_2_per_point57=state = if(below(alphax,0),0,state);
wave_2_per_point58=
wave_2_per_point59=
wave_2_per_point60=s = sample*3.14*100;
wave_2_per_point61=ss = sample*6.28*1000;
wave_2_per_point62=
wave_2_per_point63=//draw torus
wave_2_per_point64=xs = (burst*0.8 + 0.4*burst*cos(s))*cos(ss);
wave_2_per_point65=ys = (burst*0.8 + 0.4*burst*cos(s))*sin(ss);
wave_2_per_point66=zs = 0.4*burst*sin(s);
wave_2_per_point67=
wave_2_per_point68=
wave_2_per_point69=//rotate x axis
wave_2_per_point70=angle = sin(-q1*0.015)*6.28;
wave_2_per_point71=yx = ys*cos(angle) - zs*sin(angle);
wave_2_per_point72=zx = ys*sin(angle) + zs*cos(angle);
wave_2_per_point73=xx = xs;
wave_2_per_point74=
wave_2_per_point75=//rotate y axis
wave_2_per_point76=angle2 = sin(q1*0.01579)*6.28;
wave_2_per_point77=xd = xx*cos(angle2) - zx*sin(angle2);
wave_2_per_point78=zd = xx*sin(angle2) + zx*cos(angle2);
wave_2_per_point79=yd = yx;
wave_2_per_point80=
wave_2_per_point81=//rotaye z axis
wave_2_per_point82=angle3 = sin(q1*0.022)*6.28;
wave_2_per_point83=xn = xd*cos(angle3) - yd*sin(angle3);
wave_2_per_point84=yn = xd*sin(angle3) + yd*cos(angle3);
wave_2_per_point85=
wave_2_per_point86=zd = zd + 2;
wave_2_per_point87=
wave_2_per_point88=x = xn*zd*0.3 + 0.5;
wave_2_per_point89=y = yn*zd*0.3*1.2;
wave_2_per_point90=
wave_2_per_point91=
wave_2_per_point92=x = x + xdriftinc;
wave_2_per_point93=y = y + sin(yval*1.5) - 0.18;
wave_2_per_point94=
wave_2_per_point95=
wave_2_per_point96=r = 0.5 + 0.5*sin(q1*1.27 + x + x);
wave_2_per_point97=g = 0.5 + 0.5*sin(q1*1.5 + x + y);
wave_2_per_point98=b = 0.5 + 0.5*sin(q1*1.346 + y + y);
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=0
wavecode_3_bAdditive=1
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_point1=//apply zoom burst on beat
wave_3_per_point2=flag = above(q3,2);
wave_3_per_point3=//state zero is ready state
wave_3_per_point4=state = state + flag*equal(state,0);
wave_3_per_point5=
wave_3_per_point6=//upwards flight
wave_3_per_point7=yval = if(equal(state,0),0, yval);
wave_3_per_point8=yval = yval + 0.00004*equal(state,1);
wave_3_per_point9=ymax = if(equal(state,0),rand(100)*0.004,ymax);
wave_3_per_point10=
wave_3_per_point11=//hit apogee
wave_3_per_point12=state = if(above(yval,0.5+ymax),2,state);
wave_3_per_point13=
wave_3_per_point14=//reset variable
wave_3_per_point15=yval = if(equal(state,0),0, yval);
wave_3_per_point16=burst = if(equal(state,0),0.001,burst);
wave_3_per_point17=alphax = if(equal(state,0),1,alphax);
wave_3_per_point18=xdriftinc = if(equal(state,0),0,xdriftinc);
wave_3_per_point19=
wave_3_per_point20=burstspeed = if(equal(state,0),rand(10),burstspeed);
wave_3_per_point21=xdrift = if(equal(state,0),rand(20),xdrift);
wave_3_per_point22=//to get the numbers small enough have to use constants
wave_3_per_point23=xdriftinc = xdriftinc
wave_3_per_point24=+ equal(xdrift,0)*equal(state,1)*0.00002
wave_3_per_point25=+ equal(xdrift,1)*equal(state,1)*0.000018
wave_3_per_point26=+ equal(xdrift,2)*equal(state,1)*0.000016
wave_3_per_point27=+ equal(xdrift,3)*equal(state,1)*0.000014
wave_3_per_point28=+ equal(xdrift,4)*equal(state,1)*0.000012
wave_3_per_point29=+ equal(xdrift,5)*equal(state,1)*0.00001
wave_3_per_point30=+ equal(xdrift,6)*equal(state,1)*0.000008
wave_3_per_point31=+ equal(xdrift,7)*equal(state,1)*0.000006
wave_3_per_point32=+ equal(xdrift,8)*equal(state,1)*0.000004
wave_3_per_point33=+ equal(xdrift,9)*equal(state,1)*0.000002
wave_3_per_point34=+ equal(xdrift,11)*equal(state,1)*-0.000002
wave_3_per_point35=+ equal(xdrift,12)*equal(state,1)*-0.000004
wave_3_per_point36=+ equal(xdrift,13)*equal(state,1)*-0.000006
wave_3_per_point37=+ equal(xdrift,14)*equal(state,1)*-0.000008
wave_3_per_point38=+ equal(xdrift,15)*equal(state,1)*-0.00001
wave_3_per_point39=+ equal(xdrift,16)*equal(state,1)*-0.000012
wave_3_per_point40=+ equal(xdrift,17)*equal(state,1)*-0.000014
wave_3_per_point41=+ equal(xdrift,18)*equal(state,1)*-0.000016
wave_3_per_point42=+ equal(xdrift,19)*equal(state,1)*-0.000018;
wave_3_per_point43=
wave_3_per_point44=burst = burst
wave_3_per_point45=+ equal(burstspeed,0)*equal(state,2)*0.000024
wave_3_per_point46=+ equal(burstspeed,1)*equal(state,2)*0.000022
wave_3_per_point47=+ equal(burstspeed,2)*equal(state,2)*0.00002
wave_3_per_point48=+ equal(burstspeed,3)*equal(state,2)*0.000018
wave_3_per_point49=+ equal(burstspeed,4)*equal(state,2)*0.000016
wave_3_per_point50=+ equal(burstspeed,5)*equal(state,2)*0.000014
wave_3_per_point51=+ equal(burstspeed,6)*equal(state,2)*0.000012
wave_3_per_point52=+ equal(burstspeed,7)*equal(state,2)*0.00001
wave_3_per_point53=+ equal(burstspeed,8)*equal(state,2)*0.000008
wave_3_per_point54=+ equal(burstspeed,9)*equal(state,2)*0.000008;
wave_3_per_point55=
wave_3_per_point56=alphax = alphax - 0.00004*equal(state,2);
wave_3_per_point57=state = if(below(alphax,0),0,state);
wave_3_per_point58=
wave_3_per_point59=
wave_3_per_point60=s = sample*3.14*100;
wave_3_per_point61=ss = sample*6.28*1000;
wave_3_per_point62=
wave_3_per_point63=//draw torus
wave_3_per_point64=xs = (burst + 0.0001*cos(s))*cos(ss);
wave_3_per_point65=ys = (burst + 0.0001*cos(s))*sin(ss);
wave_3_per_point66=zs = 0.1*burst*sin(s);
wave_3_per_point67=
wave_3_per_point68=
wave_3_per_point69=//rotate x axis
wave_3_per_point70=angle = sin(-q1*0.035)*6.28;
wave_3_per_point71=yx = ys*cos(angle) - zs*sin(angle);
wave_3_per_point72=zx = ys*sin(angle) + zs*cos(angle);
wave_3_per_point73=xx = xs;
wave_3_per_point74=
wave_3_per_point75=//rotate y axis
wave_3_per_point76=angle2 = sin(-q1*0.03)*6.28;
wave_3_per_point77=xd = xx*cos(angle2) - zx*sin(angle2);
wave_3_per_point78=zd = xx*sin(angle2) + zx*cos(angle2);
wave_3_per_point79=yd = yx;
wave_3_per_point80=
wave_3_per_point81=//rotaye z axis
wave_3_per_point82=angle3 = sin(-q1*0.022)*6.28;
wave_3_per_point83=xn = xd*cos(angle3) - yd*sin(angle3);
wave_3_per_point84=yn = xd*sin(angle3) + yd*cos(angle3);
wave_3_per_point85=
wave_3_per_point86=zd = zd + 2;
wave_3_per_point87=
wave_3_per_point88=x = xn*zd*0.3 + 0.5;
wave_3_per_point89=y = yn*zd*0.3*1.2;
wave_3_per_point90=
wave_3_per_point91=
wave_3_per_point92=x = x + xdriftinc;
wave_3_per_point93=y = y + sin(yval*1.5) - 0.18;
wave_3_per_point94=
wave_3_per_point95=
wave_3_per_point96=r = 0.5 + 0.5*sin(q1*1.3 + x + x);
wave_3_per_point97=g = 0.5 + 0.5*sin(q1*1.1 + x + y);
wave_3_per_point98=b = 0.5 + 0.5*sin(q1*1.66 + y + y);
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=2.66718
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=0.45112
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=0.000
shapecode_0_a=0.200
shapecode_0_r2=0.000
shapecode_0_g2=0.000
shapecode_0_b2=0.000
shapecode_0_a2=0.200
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.100
shapecode_1_enabled=1
shapecode_1_sides=100
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=1
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=2.38096
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=0.42497
shapecode_1_r=0.000
shapecode_1_g=0.000
shapecode_1_b=1.000
shapecode_1_a=0.600
shapecode_1_r2=0.000
shapecode_1_g2=0.000
shapecode_1_b2=0.000
shapecode_1_a2=0.600
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=1.000
shape_1_per_frame1=r = 0.1 + 0.5*sin(q1);
shape_1_per_frame2=g = 0.1 + 0.5*sin(q1*0.9878);
shape_1_per_frame3=b = 0.1 + 0.5*sin(q1*0.897);
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.10000
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=1.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
per_frame_init_1=state = 0;
per_frame_1=basstime = basstime + bass*0.06;
per_frame_2=q1 = basstime;
per_frame_3=
per_frame_4=basstime = if(below(basstime,1000),1000,basstime);
per_frame_5=
per_frame_6=vol = pow(bass+mid+treb,2);
per_frame_7=basssum = vol;
per_frame_8=
per_frame_9=stickybit = time%2;
per_frame_10=
per_frame_11=//avg vol
per_frame_12=//buffer 1
per_frame_13=volAvg = volAvg + vol*equal(stickybit,1);
per_frame_14=//number of samples 1 or framerate
per_frame_15=sample1 = sample1 + equal(stickybit,1);
per_frame_16=//buffer 2
per_frame_17=volAvg2 = volAvg2 + vol*equal(stickybit,0);
per_frame_18=//number of samples 2
per_frame_19=sample2 = sample2 + equal(stickybit,0);
per_frame_20=
per_frame_21=//transision
per_frame_22=edge = bnot(equal(bit2,stickybit));
per_frame_23=
per_frame_24=volAvg = volAvg - volAvg*edge*stickybit;
per_frame_25=volAvg2 = volAvg2 - volAvg2*edge*equal(stickybit,0);
per_frame_26=
per_frame_27=sample1 = sample1  - sample1*edge*stickybit;
per_frame_28=sample2 = sample2  - sample2*edge*equal(stickybit,0);
per_frame_29=
per_frame_30=//test vol against avg buffer lvl
per_frame_31=diff = if(equal(stickybit,1), (basssum/(volAvg2/sample2)) , 0);
per_frame_32=diff = if(equal(stickybit,0), (basssum/(volAvg/sample1)), diff);
per_frame_33=
per_frame_34=q3 = diff;
per_frame_35=
per_frame_36=bit2 = time%2;
per_frame_37=
per_frame_38=difftime = difftime + diff*0.03;
per_frame_39=q2 = difftime;
per_frame_40=
per_frame_41=//fix a strange error
per_frame_42=difftime = if(above(difftime,2000),0, difftime);
per_frame_43=
per_pixel_1=zoom = 1;
warp_1=`shader_body
warp_2=`{
warp_3=`
warp_4=`    float3 txr = float3(uv,q1*0.1);
warp_5=`    float2  uv2 =  uv;
warp_6=`    uv2 = uv + texsize.zx*(q3,q3);
warp_7=`    float3 color = tex2D(sampler_noise_lq, uv2) - 0.5; 
warp_8=`    color += tex2D(sampler_noise_mq, uv2) - 0.5; 
warp_9=`    color += tex2D(sampler_noise_hq, uv2) - 0.5; 
warp_10=`    uv += color*0.01; 
warp_11=`
warp_12=`    ret = tex2D( sampler_main, uv).xyz;  
warp_13=`    ret = ret-0.001;// - 0.08; //or try: ret -= 0.004;
warp_14=`}
comp_1=`
comp_2=`shader_body
comp_3=`{
comp_4=`    float2 uv_echo = (uv - 0.5)*float2(-1,1) + 0.5;
comp_5=`    ret = lerp( tex2D(sampler_main, (uv-0.5)*0.98 + 0.5).xyz, 
comp_6=`                tex2D(sampler_main, (uv_echo-0.5)*0.98 + 0.5).xyz, 
comp_7=`                0.50 
comp_8=`              )  + GetBlur3(uv) + GetBlur3(uv_echo)
comp_9=`              + GetBlur1(uv) + GetBlur1(uv_echo); //video echo; //video echo
comp_10=`    ret *= 10.00; //gamma
comp_11=`    //ret =  ret*(1 - ret)*10; //brighten
comp_12=`}
