
             Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                              for Personal NetWare


 Contents
 -------- 
      - Introduction
      - Getting Started


 Introduction
 ------------ 
        The ODI driver program allows you to run multiple protocol
        stacks and install up to two network adapters in a workstation.
        This ODI driver supports the Port, Node Address, Protocol and
        Frame options for creating your own NET.CFG file. For more
        information on these keywords, please refer to Novell's
        "NetWare ODI shell for DOS - NET.CFG options". This installation
        assumes that the drivers are working properly.


 Getting Started
 --------------- 
    The NOVELL Personal NetWare installation diskettes are needed to
    complete this install.

        1. Follow the normal installation procedure as described by
           Personal NetWare.
        2. It will prompt the user for a network driver choose "Other
           Network support driver".
        3. It will request a path for the drivers. Respond with the
           path of the ODI DOS driver and NET.CFG sample installed
           with this readme.
        4. After completion of the installation procedure, modify the
           following lines in your STARTNET.BAT file from:

                  LSL
                  NE2000
                  IPXODI
                  CLIENT
           to:
                  LSL
                  DLKFET
                  IPXODI
                  CLIENT

        5. Append the <PATH>\NET.CFG file to the NWCLIENT directory.
           This directory was created when you installed Personal
           NetWare .  <PATH> is the directory where NET.CFG resides.

        6. Run STARTNET to access the Novell network.



         Parameters supported by the NET.CFG for DLKFET.COM driver
         ---------------------------------------------------------
         Protocol IPX
         Bind #1

         Link Driver DLKFET
         frame Ethernet_802.3
         ;frame Ethernet_802.2
         ;frame Ethernet_II 
         ;frame Ethernet_SNAP

         Protocol IPX 00 Ethernet_802.3
         ;Protocol IPX E0 Ethernet_802.2
         ;Protocol IPX 8137 Ethernet_II
         ;Protocol IPX 8137 Ethernet_SNAP

         ;Optional driver keywords:
         ;--------------------------------
         AUTOSENSE           ;Autosense media type
         ;10BaseT            ;Force the driver to 10Mbps half duplex mode.
         ;10BaseTFD          ;Force the driver to 10Mbps full duplex mode.
         ;100BaseTX          ;Force the driver to 100Mbps half duplex mode.
         ;100BaseTXFD        ;Force the driver to 100Mbps full duplex mode.

