1. Before Using the Printer

1.1. Packing List

When you open the package, make sure that the following parts are included in the carton:

Parts | Name | Quantity
| Printer | 1
| Laser Toner Cartridge | 1
| USB Interface Cable | 1
| Power Cord | 1
| CD-ROM | 1
| Quick Setup Guide | 1
| Pantum Warranty | 1

| Note: | • The Pantum Warranty may not be attached in some regions.

1.2. Product View

Side view

1 | Output Bin | For storing the printed paper
2 | Control Panel | To indicate the printer status and conduct the print settings operation
3 | Output Tray | To prevent the printed paper from falling
4 | Front Cover | To open the front cover to take out the laser toner cartridge
5 | Multipurpose Input Tray | To open the front cover of the multipurpose input tray, and put in the print media
6 | Multipurpose Input Tray Guide | To adjust the width of the both sides of the paper
7 | Main Power Switch | To turn on or turn off the power supply
8 | Standard Input Tray | To hold the print paper
9 | Paper-width Guide | To adjust the width of the paper inside the standard input tray

Rear view

1 | USB Interface | For directly connecting with the computer
2 | Network Interface | For connecting the printer to the network
3 | Power Interface | For connecting the power cord
4 | Rear Cover | To be opened for checking the jammed paper
5 | Duplex Printing Unit | For releasing jammed paper at the rear during duplex printing

| Note: | • The illustration may vary with different models and features, please prevail in kind.

1.3. Laser Toner Cartridge

Service Life of the Laser Toner Cartridge

Type | Average Print Volume
Laser Toner Cartridge with Standard Capacity | About 3,000 pages (The volume is based on ISO/IEC 19752 standard)
Laser Toner Cartridge with High Capacity | About 6,000 pages (The volume is based on ISO/IEC 19752 standard)
Laser Toner Cartridge with Ultra-high Capacity | About 10,000 pages (The volume is based on ISO/IEC 19752 standard)

| Note: | • The model is subject to volume increase without prior notice. • Consumables capacity may vary depending on the different types used. • We do not recommend using consumables other than that of the original Pantum consumables. • Any damages caused by using non-Pantum original consumables are not covered by the Warranty. • The appearances of laser toner cartridges will vary with different types, illustrations are for reference only.

1.4. Control Panel

1. Layout and Functions of Control Panel

The layout of the printer control panel is shown below:

No. | Name | Functions
1 | LCD Display | The display provides information about the printer and can be used for setting up the Product Settings.
2 | UP | Press this button to browse through each menu and its options. For menu items need to input, change the numeric value by cycle accumulating.
3 | Menu | Open the main menu of the control panel to conduct the menu setting.
4 | Down | Press this button to browse through each menu and its options. For menu items need to input, move the position of the cursor, e.g., IP address input.
5 | Wi-Fi/Configuration Report | This button can enable the Wi-Fi feature and indicate the Wi-Fi connection status (only applicable to Wi-Fi model). For non-Wi-Fi model, this button will be used to print the "Printer Information Page" and the "Network Configuration Report".
6 | OK | • Press this button to save the settings. • Open the submenu on the display of the control panel. • Select the menu item.
7 | Back | Back Arrow Button: use this button to perform the following operations: • Exit the control panel menu. • Scroll back to the previous menu in the list in the submenu. • Return to the previous menu; if already at the top menu, return to the Ready interface.
8 | Cancel | Press this button to cancel the operation. Cancel the current printing operation if there is any.
9 | Status Indicator | This light indicates the ready, alarm and other statuses of the printer. Green light: Normal. Orange light: Alarm or cartridge toner level is low. Red light: Error.
10 | Power Indicator | Green for starting up, working, and sleeping; while staying on indicates the power supply is ready

2. Status Indicator

The multi-colored LED indicator will display red, orange and green with the specific meanings as follows:

| Red indicates the emergence of a serious error, such as the laser toner cartridge is not installed, the laser toner cartridge does not match the printer, or the paper tray is out of paper; and in such a case, it will keep the red light on. For specific error, see Chapter 9 Troubleshooting.
| The display provides information about the printer and can be used for setting up the Product Settings.
| Press this button to browse through each menu and its options. For menu items need to input, change the numeric value by cycle accumulating.

1.5. Print the Product Report

Users can print the product report by manipulating the control panel. These pages can help you understand the product information, diagnose and resolve product failures.

1) Press "Menu" to enter the Menu Settings interface.

2) Press direction key "▲" or "▼" to select the "5.Prt Info Rept" option.

3) Press "OK" to enter the Print Information Report interface, and users can print the product report according to their needs.

| Note: | • In case of non-Wi-Fi model, users can also print the network configuration report of the printer directly through the shortcut button of "Network Configuration Report" on the control panel.