> ### Measuring Vertex Coordinates

> The Vertex Coordinates option provides the coordinates of vertices on the model.

> 1. From the Markup menu, select Add Entity, and then select Vertex Coordinate.

> The Measurement Entities dialog box appears.

> Note: From the Markup Entity toolbar, you can also click Vertex Coordinate .

> Note: All vertices on the model are highlighted.

> 2. Scroll over the vertex whose coordinates you want to add to the markup.

> The X, Y, and Z coordinates appear in a tooltip.

> 3. Click the vertex.

> The X, Y, an Z coordinates and unit appear a value box entity on the current active markup layer and in the Measurement Entities dialog box.

> 4. Click and drag the value box anywhere on the markup.

> Click and drag the frame handles to enlarge the value box.

> Note: Click Reset to take another measurement.

> 5. To remove the highlighted vertices on the model, click Close in the Measurement Entities dialog box.

> See Also Changing Measurement Units and Symbols

> Changing Font

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers