> ## Design Verification

> Design verifications are operations that check the electrical design of a PCB against a set of rules defining physical and electrical design limitations. Performing these checks will prevent short circuits and process errors. The types of design rules are as follows:

> - Clearances - The minimum spacing (air gaps) allowed between two sets of entities in the design. These sets can belong to the same type of entity or to different types.
> - Electrical - Targets certain properties of the nets
> - Manufacturing - Targets the physical properties of a particular entity.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers