> ## Angle in Vector Files

> Use the Angle option to measure the angle between points on a drawing.

> 1. From the Analysis menu, select Measure.

> The Measurement dialog box appears.

> Note: From the AutoVue toolbar, you can also click Measure .

> 2. Click the Angle tab.
> 3. Select From 3 Points if you want to measure the angle between three points.
>    Snapping modes are displayed.
> 4. Select the snapping modes that you want to use for measuring.

> To select all snapping modes click All On. To deselect all snapping modes click All Off.

> See 2D Vector Snapping Modes

> 5. Select Between 2 lines if you want to measure the angle between two lines.
> 6. From the Measured Angle Units list, select the unit.
> 7. If you selected From 3 Points, click three points on the drawing to define the angle.
> 8. If you selected Between 2 Lines, click two lines on the drawing to define the angle.

> Angle arms appear with an arc connecting them. The angle measurement appears in the Measurement dialog box.

> Note: Click Reset to take another measurement.

> 9. Click Close to close the Measurement dialog box.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers