> ## Rotating a Model Along the X, Y and Z-Axis

> 1. From the Manipulate menu, select Manipulate.
>    You are now in Manipulate mode.

> Note: From the AutoVue toolbar, you can also click Manipulate .

> 2. Select the model part or parts that you want to manipulate.

> Note: To select more than one part, press the Shift or Control key when selecting.

> A model-size representation of the Global Axes appears through the model part or parts and are enclosed by a three-dimensional box.

> 3. Click and hold the mouse button on the sphere at the end of the axis you want to rotate.

> Clicking on an axis sphere allows rotation around one of the other two axes.

> Note: The initial mouse movement determines which of the two axes will mark the site of rotation. If the axis you chose does not rotate around the right axis for the rotation that you want to make, click the sphere again and move the mouse in a different direction.

> 4. Move the mouse to rotate the model by the selected axis.

> Note: If you want to rotate the selection freely, as done in Rotate Mode, press the Control key during rotation.

> 5. To exit Manipulate mode, click Manipulate , or from the Manipulate menu, select Manipulate.

> Note: To restore the default state of a part of the model, from the Manipulate menu, select Transform, and then select Reset Selected. To restore the default state for the whole model, select Reset All.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers