> ### Modifying an Overlay

> 1. From the Manipulate menu, select Overlays.

> The Modify Overlay dialog box appears.

> 2. Select the overlay that you want to modify.
> 3. Click the Action that you want to apply to the overlay.
> - Click Move if you want to move the overlay.
>   Click a point on the base file where you want to set the lower left corner of the overlay. Click another point where you want to set the upper right corner of the overlay.

> Note: As you select the point to define the position of the upper right corner, you can resize the destination box.

> - Click Scale if you want to resize the overlay.
>   Enter the XOffset and YOffset coordinates and/or the Scale Factor.

> Note: XOffset and YOffset are relative to the base drawing and all options are displayed at their current values.

> - Click Warp to adjust the overlay.
>   Click a point on the overlay and drag the cursor to where you want the overlay starting point. Click another point and drag the cursor to where you want the overlay to end.

> Note: The overlay’s size is scaled to accommodate the origin and destination points you defined.

> 4. Click OK.

> The changes are applied to the selected overlay.

> Note: To modify other overlays, repeat steps 2 to 4.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers