> ## Measuring Vertex Coordinates

> The Vertex Coordinates option provides the coordinates of vertices on the model.

> 1. From the Analysis menu, select Measure.

> The Measurement dialog box appears.

> Note: From the AutoVue toolbar, you can also click Measure .

> 2. Click the Vertex tab.

> All vertices on the model are highlighted.

> 3. From the Coordinates Units list, select the unit in which you want to measure.
> 4. Move the cursor over the highlighted vertex that you want to measure.

> The X, Y and Z coordinates appear in a tooltip.

> 5. Select the vertex.

> The X, Y an Z coordinates appear in the Measurement dialog box.

> Note: Click Reset to take another measurement.

> 6. Click Close the close the Measurement dialog box.

http://www.oracle.com/applications/autovue/index.html Voice: (514) 735-3219 Fax: (514) 735-6440 info@cimmetry.com Copyright © 1989, 2008, Oracle and/or its affiliates. All rights reserved. Notices and disclaimers