;Windows Modem Setup File
;Copyright 1995-1999 Microsoft Corp. \\MS-IRL\\
;Manufacturer:   LASAT COMMUNICATIONS A/S
[Version]
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
LayoutFile=layout.inf
DriverVer=07/01/2001,5.1.2535.0

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%Mfg% = Lasat

[Lasat]
%Modem21%=Modem21,*LASF441
%Modem20PnP%=Modem20,SERENUM\LASC040
%Modem19%=Modem19,PCMCIA\LASAT_COMMUNICATIONS_A/S-LASAT_Credit_560_Voice-6D7E  ;V90
%Modem18PnP%=Modem18,SERENUM\LASC044
%Modem17PnP%=Modem17,SERENUM\LASF444
%Modem16%=Modem16,PCMCIA\LASAT_COMMUNICATIONS_A/S-LASAT_CREDIT_336-CF2C
%Modem16%=Modem16,PCMCIA\LASAT_COMMUNICATIONS_A/S-LASAT_CREDIT_336-0134-3611
%Modem15PnP%=Modem15,SERENUM\LAS4540
%Modem14PnP%=Modem14,SERENUM\LAS5440
%Modem13PnP%=Modem13,SERENUM\LAS4040
%Modem6%=Modem6,PCMCIA\LASAT_COMMUNICATIONS_A/S-LASAT_CREDIT_288-BD1B  
%Modem6%=Modem6,PCMCIA\LASAT_COMMUNICATIONS_A/S-LASAT_CREDIT_288-0AFE  
[Modem21]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem20.AddReg,Internal,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG ,Lasat_voice
[Modem20]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem20.AddReg,External,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG ,Lasat_voice
[Modem19]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem19.AddReg,PCMCIA,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG ,Lasat_voice
[Modem18]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem18.AddReg,External,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG ,Lasat_voice
[Modem17]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem17.AddReg,External,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG ,Lasat_voice
[Modem16]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgaddReg,Modem16.AddReg,PCMCIA,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG 
[Modem15]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg ,Modem15.AddReg,External,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG 
[Modem14]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg,Modem14.AddReg,External,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG 
[Modem13]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf 
AddReg=All,MfgAddReg,Modem13.AddReg,External ,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG 
[Modem6]
DriverVer=06/01/1999,5.00.0000.0
include=mdmgl010.inf
AddReg=All,MfgAddReg,Modem6.AddReg,PCMCIA ,MDMGL010.V34LONG,MDMGL010.NUMERICS,MDMGL010.V34SHORT,MDMGL010.ALL,MDMGL010.V90SHORT,MDMGL010.V90LONG 
[Modem19.Addreg]
HKR,,Properties,1,80,01,00,00,ff,00,00,00,ff,00,00,00,07,00,00,00,0F,00,00,00,FF,03,00,00,00,c2,01,00,C0,DA,00,00
HKR,,VoiceProfile,1,A1,12,19,02
HKR,,PowerDelay,0x10001,1500
HKR,,ConfigDelay,0x10001,1500
HKR,Settings,ErrorControl_Cellular,,"\N3-K1*H1)M1-Q0"
HKR,Settings,ErrorControl_Cellular_Forced,,"\N2-K1*H1)M1-Q0"
[Modem18.Addreg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,60,EA,00,00
HKR,,VoiceProfile,1,A1,12,19,02
HKR,Settings,DialSuffix,,";"
[Modem20.Addreg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,60,EA,00,00
HKR,,VoiceProfile,1,A1,12,19,02
HKR,Settings,DialSuffix,,";"
[Modem17.Addreg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,60,EA,00,00
HKR,,VoiceProfile,1,E5,12,19,02
HKR,Settings,DialSuffix,,";"
[Modem16.AddReg]
HKR,,Properties,1,80,01,00,00,ff,00,00,00,ff,00,00,00,07,00,00,00,0f,00,00,00,ff,03,00,00,00,c2,01,00,80,70,00,00
HKR,Settings,ErrorControl_Cellular,,"\N3-K1*H1)M1-Q0"
HKR,Settings,ErrorControl_Cellular_Forced,,"\N2-K1*H1)M1-Q0"
[Modem13.AddReg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,40,83,00,00
[Modem14.AddReg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,40,83,00,00
[Modem15.Addreg]
HKR,,Properties,1,80,01,00,00,FF,00,00,00,FF,00,00,00,07,00,00,00,0F,00,00,00,F7,03,00,00,00,C2,01,00,60,EA,00,00
[Modem6.AddReg] ; CREDIT 288
HKR,,Properties,1,80,01,00,00,ff,00,00,00,ff,00,00,00,07,00,00,00,0f,00,00,00,ff,03,00,00,00,c2,01,00,80,70,00,00
HKR,Settings,ErrorControl_Cellular,,"-K1"
HKR,Settings,ErrorControl_Cellular_Forced,,"-K1)M1"
[Strings]
Mfg="Lasat"
MSFT="Microsoft"
Modem21="Lasat 560 V Int"
Modem20PnP="Lasat Websetgo 56 Voice PnP"
Modem19="Lasat Credit 560 Voice K56Flex & V.90"
Modem18PnP="Lasat Internet 560 Voice PnP"
Modem17PnP="Lasat Safire 560 Voice PnP"
Modem16="Lasat Credit 336"
Modem15PnP="Lasat Safire 560 PnP"
Modem14PnP="Lasat Safire 336  PnP"
Modem13PnP="LASAT Internet 33600 PnP"
Modem6="LASAT CREDIT 288"
[All]
HKR,,FriendlyDriver,,Unimodem.vxd
HKR,,DevLoader,,*VCOMM
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
[EXTERNAL]
HKR,,DeviceType,1,01
[INTERNAL]
HKR,,DeviceType,1,02
[PCMCIA]
HKR,,PortDriver,,Serial.vxd
HKR,,Contention,,*vcd
HKR,,DeviceType,1,03
[MfgAddReg]
HKR,Init,1,,"AT<cr>"
HKR,Init,2,,"AT&F E0 V1 &S0 &C1 &D2 W2 S95=47 S0=0<cr>"
HKR,Monitor, 1,,"ATS0=0<cr>"
HKR,Monitor, 2,,"None"
HKR,Hangup,1,,"ATH<cr>"
HKR,Answer,1,,"ATA<cr>"
HKR,,Reset,,"AT&F<cr>"
HKR,,InactivityScale,1,0a,00,00,00
HKR,Settings,Prefix,,"AT"
HKR,Settings,Terminator,,"<cr>"
HKR,Settings,DialPrefix,,"D"
HKR,Settings,DialSuffix,,""
HKR,Settings,SpeakerVolume_Low,,"L0"
HKR,Settings,SpeakerVolume_Med,,"L2"
HKR,Settings,SpeakerVolume_High,,"L3"
HKR,Settings,SpeakerMode_Off,,"M0"
HKR,Settings,SpeakerMode_Dial,,"M1"
HKR,Settings,SpeakerMode_On,,"M2"
HKR,Settings,SpeakerMode_Setup,,"M3"
HKR,Settings,FlowControl_Off,,"&K0"
HKR,Settings,FlowControl_Hard,,"&K3"
HKR,Settings,FlowControl_Soft,,"&K4"
HKR,Settings,ErrorControl_On,,"\N3"
HKR,Settings,ErrorControl_Off,,"\N0"
HKR,Settings,ErrorControl_Forced,,"\N2"
HKR,Settings,Compression_On,,"%%C3"
HKR,Settings,Compression_Off,,"%%C0"
HKR,Settings,Modulation_CCITT,,"B0"
HKR,Settings,Modulation_Bell,,"B1"
HKR,Settings,SpeedNegotiation_Off,,"N0"
HKR,Settings,SpeedNegotiation_On,,"N1"
HKR,Settings,Pulse,,"P"
HKR,Settings,Tone,,"T"
HKR,Settings,Blind_Off,,"X4"
HKR,Settings,Blind_On,,"X3"
HKR,Settings,CallSetupFailTimer,,"S7=<#>"
HKR,Settings,InactivityTimeout,,"S30=<#>"
[Lasat_voice]     
HKR,WaveDriver,BaudRate       ,1,00,c2,01,00
HKR,WaveDriver,XformID        ,1,01,00
HKR,WaveDriver,XformModule    ,,"umdmxfrm.dll"
HKR,WaveDriver,WaveHardwareID ,,"LASATVoiceModemWave"
HKR,,VoiceBaudRate,1,00,c2,01,00
HKR,,Enumerator,,serwave.vxd
HKR,,VoiceMixerMid, 1,16,00
HKR,,VoiceMixerPid, 1,15,00
HKR,,VoiceMixerLineID, 1,00,00,04,00
HKR,EnableCallerID,1,,"at<cr>"
HKR,,HandsetCloseDelay,1,1e,00,00,00
HKR,StartPlay,1,,"at#vtx<cr>"
HKR,StopPlay,1,,"None"
HKR,StopPlay,2,,"NoResponse"
HKR,StartRecord,1,,"at#vrx<cr>"
HKR,StopRecord, 1,,"None"
HKR,StopRecord, 2,,"NoResponse"
HKR,,TerminateRecord,,"<h10><cr>"
HKR,,TerminatePlay,,"<h10><h03>"
HKR,,AbortPlay,,"<h10><h18>"
HKR,LineSetPlayFormat,1,,"at#vls=0<cr>"
HKR,LineSetRecordFormat,1,,"None"
HKR,LineSetRecordFormat,2,,"NoResponse"
HKR,HandsetSetRecordFormat, 1,,"at#vls=3<cr>"
HKR,HandsetSetRecordFormat, 2,,"at#vsr=7200<cr>"
HKR,HandsetSetRecordFormat, 3,,"at#vbs=4<cr>"
HKR,HandsetSetPlayFormat,1,,"at#vls=2<cr>"
HKR,HandsetSetPlayFormat,2,,"at#vsr=7200<cr>"
HKR,HandsetSetPlayFormat,3,,"at#vbs=4<cr>"
HKR,OpenHandset,1,,"at#cls=8<cr>"
HKR,OpenHandset,2,,"at#vls=2<cr>"
HKR,CloseHandset,1,,"at#vls=0<cr>"
HKR,CloseHandset,2,,"at#cls=0<cr>"
HKR,VoiceToDataAnswer,1,,"at#cls=0<cr>"
HKR,VoiceToDataAnswer,2,,"ata<cr>"
HKR,VoiceAnswer,1,,"at#cls=8<cr>"
HKR,VoiceAnswer,2,,"at#vls=0<cr>"
HKR,VoiceAnswer,3,,"at#vbt=1<cr>"
HKR,VoiceAnswer,4,,"at#vsr=7200<cr>"
HKR,VoiceAnswer,5,,"at#vbs=4<cr>"
HKR,VoiceAnswer,6,,"ats30=60<cr>"
HKR,VoiceAnswer,7,,"ata<cr>"
HKR,VoiceDialNumberSetup,1,,"at#cls=8<cr>"
HKR,VoiceDialNumberSetup,2,,"at#vls=0<cr>"
HKR,VoiceDialNumberSetup,3,,"at#vrn=0<cr>"
HKR,VoiceDialNumberSetup,4,,"at#vbt=1<cr>"
HKR,VoiceDialNumberSetup,5,,"at#vsr=7200<cr>"
HKR,VoiceDialNumberSetup,6,,"at#vbs=4<cr>"
HKR,VoiceDialNumberSetup,7,,"ats30=60<cr>"
HKR,GenerateDigit,1,,"at#vts=<Digit><cr>"
HKR,,CallerIDPrivate,,P
HKR,,CallerIDOutSide,,O
HKR,,VariableTerminator,,<cr><lf>
HKR,EnableDistinctiveRing,1,,"at-sdr=7<cr>"
HKR,,ForwardDelay, 1,88,13
HKR,Responses,"<cr><lf>VCON<cr><lf>",1,00,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>DATE = ",1,93,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>TIME = ",1,94,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NMBR = ",1,95,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>NAME = ",1,96,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>MESG = ",1,97,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING1<cr><lf>",1,18,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING2<cr><lf>",1,19,00,00,00,00,00,00,00,00,00
HKR,Responses,"<cr><lf>RING3<cr><lf>",1,1a,00,00,00,00,00,00,00,00,00
HKR,,SpeakerPhoneSpecs,1,0A,00,00,00,0f,00,00,00,03,00,00,00,00,00,00,00
HKR,SpeakerPhoneEnable,1,,"at#cls=8<cr>"
HKR,SpeakerPhoneEnable,2,,"at#vls=6<cr>"
HKR,SpeakerPhoneEnable,3,,"at#spk=1,10,2<cr>"
HKR,SpeakerPhoneDisable,1,,"at#spk=0,16,,<cr>"
HKR,SpeakerPhoneDisable,2,,"at#vls=0<cr>"
HKR,SpeakerPhoneMute,1,,"at#vls=6<cr>"
HKR,SpeakerPhoneMute,2,,"at#spk=0,,,<cr>"
HKR,SpeakerPhoneUnMute,1,,"at#vls=6<cr>"
HKR,SpeakerPhoneUnMute,2,,"at#spk=1,,,<cr>"
HKR,SpeakerPhoneSetVolumeGain,1,,"at#vls=6<cr>"
HKR,SpeakerPhoneSetVolumeGain,2,,"at#spk=,<Vol>,<Gain><cr>"
