### Backup

#### RGDV related Assignments

#### RGDV 1...8

APR Assignments After Reading (spinning bar) the PC offers the default backup name
Backup File Name: APR_BAK1...8.TDL.
The default name can be changed into any other (up to 8 digit) file name.
The path from which XRGSCOPE has been started on the hard disk will automatically be taken into account.
It is also possible to type A:\filename <ENTER> to load the backup file directly to a floppy disk.

### CU Complete

The default backup name Backup File Name: CUBACKUP.TDL (or A:\filename <ENTER>) can be changed into any other (up to 8 digit) file name (e.g. CU97xxxx.TDL representing the generator serial number). A disk space of 700 kByte is required. It takes about 8...15 minutes to save the data to the floppy / hard disk.
The path (from which XRGSCOPE has been started on the hard disk) will automatically be taken into account.
It is also possible to type A:\filename <ENTER> to load the backup file directly to a floppy disk.