Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00M3 | Error/Warning |
Description:
No response at all from FU(s) #1H, #2H, #3H, #4H, #5H, #6H. The unit(s) will be indicated in the string at #1H, #2H ... , all other fields will indicate 00H
Possible Causes / Advice:
Click here for list of Functional Units Check if FCO 00 135 004 (high speed rotor control modification) has been carried out.