Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00SJ | Error |
Description:
PCcomm: Syntax wrong
Possible Causes / Advice:
This error will occur when you are uploading or downloading data from the PC and the signal bus (EZ-X42 & EZ-X42) and the signal bus (EZ-X23) are not disconnected. Disconnect these cables and try again. PC Up/Download Procedure