Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00XP | Error/Warning |
Description:
exposure time too long
Possible Causes / Advice:
Most likely in free techniques without AEC, FU_mA terminates non-AEC exposures once the set mAs is achieved, if X_ACT_S/ has not been received as mAs counter trigger or if STOP_X_C/ has not been sent by FU_mA CU terminates the exposure.