Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00BS | Error/Warning |
Description:
APR: The RGDV of the APR is not ready for operation
Possible Causes / Advice:
This error will occur when attempting to upload APRs to a Registartion Device that is not configured in the Optimus. (i.e. Bucky TH without tomo and you attempt to load the tomo APRs for RDGV 2.)