Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00XU | Warning |
Description:
Input message filed out of range
Possible Causes / Advice:
This error can happen during the transition from fluoro to exposure, Scopomat exposures only,solved with Release 3.5. The SW can be upgraded with FCO74200002. This FCO is "Retrofit on Failure" so it will not automatically come to the site.