### Restore

#### RGDV1...8

APR Assignments The path (from which XRGSCOPE has been started on the hard disk) will automatically be taken into account or type in either A:\filename <ENTER> or just A: <ENTER>, <TAB> and select a file with the cursor up/down buttons.

Load Data from Disk: will offer the default file name APR_BAK1...8.

#### CU Complete

Load Data from Disk offers the default File Name: CUBACKUP.TDL (taking the path from which XRGSCOPE has been started automatically into account) or type in either A:\filename <ENTER> or just A: <ENTER>, <TAB> and select a file with the cursor up/down buttons.

It takes about 15-30 minutes to restore the data (PC type dependent). If the spinning bar during the loading procedure seem to turn very slowly then stop the procedure.

Date and Time must be set after restore is finished with a new PCB CU or after the NVRAM has been erased by pulling the battery jumper.