Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00I4 | Error/Warning |
Description:
One FU (Functional Unit) has a Watch Dog-error A message with an unexpected message number (Internal Interface Message) has been received, the first parameter byte gives the Internal Interface Message that was received.
Possible Causes / Advice:
scantime_TV is not programmed correctly. Check: XRGSCOPE -->OPTIMUS --> Program --> Dose rate control --> CONT: scantime_TV = 20.00 ms