Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00X6 | Error/Warning |
Description:
timeout setting FUs, response missing
Possible Causes / Advice:
If this error intermittently occurs after prep then install R3.5 SW with FCO 74200002. This FCO is "Retrofit on Failure" so it will not automatically come to the site.