Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00CD | Warning |
Description:
The Functional Unit is not addressable on the CAN bus. Sample error message: ( xx= the Fuctional Unit that can not be addressed in HEX ) CAN: FU xxH not addressable Check for the RED light on the associated functional unit. It should be off when operating properly. If not investigate further. Click here for list of Functional Units
Possible Causes / Advice: