Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HB | Error |
Description:
kV nominal value out of range: 0 kV > U > 170 kV
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select error details and read screen Error: HW Set Values to get kV nominal, then read Error: Specific Information to get the faulty value. Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If all supplies OK replace PCB