<module>
4X4矩阵键盘上边有16个按键, 当用户按下时就会触发“按钮按下事件”，松开的时候，触发“按钮松开事件”。
</module>
<name> Pack 矩阵键盘,
</name>
<member> var_uint16 OS_time OS_time,

</member>,
<member> var_uint16 OS_EventFlag OS_EventFlag,

</member>,
<member> var_uint16 OS_EventFlag1 OS_EventFlag1,

</member>,
<member> event key0_press_event 按键0按下时,

</member>,
<member> event key0_up_event 按键0松开时,

</member>,
<member> event key1_press_event 按键1按下时,

</member>,
<member> event key1_up_event 按键1松开时,

</member>,
<member> event key2_press_event 按键2按下时,

</member>,
<member> event key2_up_event 按键2松开时,

</member>,
<member> event key3_press_event 按键3按下时,

</member>,
<member> event key3_up_event 按键3松开时,

</member>,
<member> event key4_press_event 按键4按下时,

</member>,
<member> event key4_up_event 按键4松开时,

</member>,
<member> event key5_press_event 按键5按下时,

</member>,
<member> event key5_up_event 按键5松开时,

</member>,
<member> event key6_press_event 按键6按下时,

</member>,
<member> event key6_up_event 按键6松开时,

</member>,
<member> event key7_press_event 按键7按下时,

</member>,
<member> event key7_up_event 按键7松开时,

</member>,
<member> event key8_press_event 按键8按下时,

</member>,
<member> event key8_up_event 按键8松开时,

</member>,
<member> event key9_press_event 按键9按下时,

</member>,
<member> event key9_up_event 按键9松开时,

</member>,
<member> event keyA_press_event 按键A按下时,

</member>,
<member> event keyA_up_event 按键A松开时,

</member>,
<member> event keyB_press_event 按键B按下时,

</member>,
<member> event keyB_up_event 按键B松开时,

</member>,
<member> event keyC_press_event 按键C按下时,

</member>,
<member> event keyC_up_event 按键C松开时,

</member>,
<member> event keyD_press_event 按键D按下时,

</member>,
<member> event keyD_up_event 按键D松开时,

</member>,
<member> event keyStar_press_event 按键星号按下时,

</member>,
<member> event keyStar_up_event 按键星号松开时,

</member>,
<member> event keySharp_press_event 按键井号按下时,

</member>,
<member> event keySharp_up_event 按键井号松开时,

</member>,
<member> event keyNumber_press_event 任意数字键按下时,

</member>,
<member> event keyNumber_up_event 任意数字键松开时,

</member>,
<member> event keyAny_press_event 任意键按下时,

</member>,
<member> event keyAny_up_event 任意键松开时,

</member>,
<member> var_int32 Value 按键值,

</member>,
<member> function_void OS_init OS_init,

</member>,
<member> function_void OS_run OS_run,

</member>,
<member> function_bool_int32 is_press 第 # 个按键按下,

</member>,
