| Home > Product Information # Command Lists EPSON ESC/P-C control codes Brother M4024 emulation control codes Your printer supports the EPSON ESC/P-C control codes and Brother M4024 emulation control codes listed below. ## EPSON ESC/P-C control codes Selecting an EPSON ESC/P-C printer in your software allows you to use advanced fonts and graphics. ### ASCII mode General operation: ESC@, ESC U Paper feeding: FF, LF, ESC 0, ESC 2, ESC 3, ESC +, CR Page format: ESC ( C, ESC C, ESC C 0, ESC Q, ESC l, ESC ( c, ESC N, ESC O Print position motion: ESC $, ESC \, ESC ( V, ESC ( v, ESC D, HT, ESC B, VT, ESC J Font selection: ESC k, ESC x, ESC y, ESC X, ESC P, ESC M, ESC g, ESC p, ESC 4, ESC 5, ESC E, ESC F, ESC ! Font enhancement: ESC W, DC 4, SO, DC2, SI, ESC w, ESC G, ESC H, ESC T, ESC S, ESC -, ESC ( -, ESC q, ESC (X Spacing: ESC Space, ESC c, ESC ( U Character handling: ESC t, ESC ( t, ESC R, ESC %, ESC &, ESC :, ESC 6, ESC 7, ESC ( ^ Bit image: ESC * Barcode: ESC (B Production: ESC │ ### Hanji mode Font selection: FS &, FS ., FS k, SI, SO, ESC n, ESC o Font enhancement: FS SO, FS DC4, FS W, FS H, FS I, FS J, FS K, FS, FS D, FS SI, FS DC2, FS r, FS v, FS j, FS ! Spacing: FS S, FS T, FS U, FS V Font handling: FS x, FS 2, FS t Top ## Brother M4024 emulation control codes This printer emulates the Brother Proprinter using the commands below. General operation: ESC @, ESC A n, CAN, DC1, DC3 Paper feeding: FF, LF, ESC C n, ESC J n, CR Page format: ESC B n, ESC ( nH nL, ESC ) nH nL Print position motion: ESC 6 nH nL, VT, ESC H n, ESC I, ESC VT n, ESC Z nH nL Font enhancement: SO, SI Bit image: ESC 4 nH nL, ESC G nH nL, ESC = nH nL Top |