# Auto Firmware Update Settings
Device Management > Configuration > Device Settings > Auto Firmware Update Settings

Use this page to update the device's firmware automatically.

Note

- Settings on this page can be changed by the following administrator:
  - Machine Administrator

## Settings to Prohibit Updates

Specify when to prohibit the auto firmware update.
The firmware cannot be updated when the machine is operating. If you specify your working hours for the update prohibition period, the firmware is automatically updated during non-working hours without disturbing your work.

### Timer to Prohibit Updates

Specify whether or not to enable the prohibition period setting for the auto firmware update.
When On is selected, specify the start time and end time.

### Day of the Week to Prohibit Updates

Specify which days of the week to prohibit the auto firmware update.

## Proxy Server Settings

### Proxy Server

Select to use a proxy server for Internet connection.
To use a proxy server, select On, and then configure the following settings.
(When Off is selected, you do not need to configure the following settings.)

### Proxy Address

Enter the host name or IP address of the proxy server.

### Port Number

Enter the port number of the proxy server.
Enter from 0 to 65535. The default is 0.

### User Name

Enter the user name used when logging in to the proxy server.
You can enter up to 31 alphanumeric characters.

### Password

Click Change to change the password for logging in to the proxy server.
You can enter up to 31 alphanumeric characters.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##