# IPDS Form Settings/Add IPDS Form
Device Management > Configuration > Printer > IPDS Form Settings/Add IPDS Form

Use this page to make changes to IPDS form settings or to register new IPDS settings.

Note

- Settings on this page can be edited by the following administrator:
  - Machine Administrator

## IPDS Form Settings

Configure settings for the IPDS form.

### Form Name

Enter the name of the form, using up to 16 characters.

### Description

Enter the description for the form, using up to 90 characters. (You can leave this text box blank.)

### Media Size

Select the size of the form.

### Custom Size Units

If you select Custom for Media Size, select the unit of measurement for the custom form.

#### Cross Feed Dimension

Specify the length of the edge of the form that is fed into the printer.

#### Feed Dimension

Specify the length of the edge of the form that is NOT fed into the printer.

### Media Type

Select the type of the form.

### Media Orientation

Specify whether the media orientation is Long (long edge feed) or Short (short edge feed).

### Media Type Component ID

Specify whether or not to specify the Media Type Component ID. If you select Specify, enter the ID number using a value between 0 and 65535.

### Edge Sensitive

Specify whether or not the printer rotates the print image 180 degrees.

### Side Sensitive

Select Yes for the jobs that contain a combination of simplex (single-sided) and duplex (double-sided) pages and that require preprinted or prepunched forms.

### Simplex Only

Specify whether to perform simplex (single-sided) printing or duplex (double-sided) printing.

### Simplex Adjust Cross Feed

When performing simplex (single-sided) printing, specify the horizontal offset (relative to the paper feed orientation).

### Simplex Adjust Feed

When performing simplex (single-sided) printing, specify the vertical offset (relative to the paper feed orientation).

### Front Duplex Adjust Cross Feed

When performing duplex (double-sided) printing, specify the horizontal offset of the front page (relative to the paper feed orientation).

### Front Duplex Adjust Feed

When performing duplex (double-sided) printing, specify the vertical offset of the front page (relative to the paper feed orientation).

### Back Duplex Adjust Cross Feed

When performing duplex (double-sided) printing, specify the horizontal offset of the back page (relative to the paper feed orientation).

### Back Duplex Adjust Feed

When performing duplex (double-sided) printing, specify the vertical offset of the back page (relative to the paper feed orientation).

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

### Back

Click to return to the previous page.

##