# System
Device Management >Configuration > Device Settings > System

Configure settings for device name, output tray, priority tray, cover sheet tray, and slip sheet tray.

Note

- Settings on this page can be changed by the following administrators and users:
  - Network Administrator (Device Name, Comment, and Location)
  - Machine Administrator (Items other than Device Name, Comment, and Location)
  - Login users (all items except Protect Printer Display Panel), if:
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.
- Some items may not appear depending on machine type or configuration.

## General Settings

### Device Name

Enter the device name, using up to 31 characters.

Note

- The device name is different from the host name entered in the Host Name box on the Configuration: Network: IPv4 or Configuration: Network: IPv6 page.

### Comment

Enter a note about the machine, using up to 31 characters.

### Location

Enter the device location, using up to 32 characters.

### Spool Printing

Specify whether Spool Printing is active or inactive.
This appears only when Spool Printing is supported by the machine.

Note

- When Active is selected, you can select Job - Printer - Spool Printing. This displays the Spool Printing Job List page.
  When Inactive is selected, the Spool Printing item does not appear on the Job page.
- Spool printing is active or inactive when you click OK on this page. Job - Printer - Spool Printing is displayed or hidden when the Web browser restarts after the setting is applied.

### Protect Printer Display Panel

Specify whether to restrict access from the printer control panel, and if yes, select a protection level.
If protection is enabled, changing control panel items is not possible.
This appears only when printer function is supported by the machine.

Note

- If you select Level 1 or Level 2, the protection level that is applied is the same as that specified for Level 1 or Level 2 of the Menu Protect setting in the printer's settings, which are configured using the machine control panel.
- For details about setting Menu Protect, see the operating instructions provided with the machine.
- This item appears only when you are logged in as Machine Administrator.

### Interleave Priority

Select the priority job type for the machine.
For example, if there is a job submitted from the copier function using the machine's control panel and a job sent from a client computer, the client computer's job is printed first if Printer is selected for Interleave Priority.

Note

- Copier/Document Server, Fax, or Printer appears only if the machine supports these functions.
- This is displayed only if/when supported by the machine.

#### Display Mode

Gives priority to jobs submitted using the mode selected on the machine's control panel.

#### Switch Every Specified No. of Sheets

Gives priority to jobs submitted using the Interrupt function. The current print job is interrupted after the number of sheets specified on the machine's control panel are printed.

#### Job Order

No priority setting. Jobs are printed in the order they were submitted.

#### Copier/Document Server

Gives priority to jobs submitted using the copier function and jobs submitted from the machine's Document Server.

#### Fax

Gives priority to jobs submitted using the fax function.

#### Printer

Gives priority to jobs submitted using the printer function.

### Function Reset Timer

Specify a time period to elapse before the machine switches to the function selected in Interleave Priority.

#### Set Time

Specify how long (3 to 30 seconds) the machine waits before it switches to the selected function.

#### Immediate

The machine switches to the selected function immediately.

### Stop Key to Suspend Print Job

Select how to stop a print job when you press the "Stop" key on the machine's control panel.

#### All Jobs *1

Temporarily pauses all the jobs that are being printed. You can then specify the jobs you want to cancel in the Job Management screen on the machine's control panel.

*1: Includes jobs that enter the queue after you press the "Stop" key

#### All Jobs Being Executed *2

Temporarily pauses all the jobs that are being executed. You can then specify the jobs you want to cancel in the Job Management screen on the machine's control panel.
If there are no jobs being executed, the "Stop" key is disabled.

*2: Jobs being printed and jobs waiting to be printed

#### Only Job Being Operated

Only jobs that are being processed are canceled.

### Display IP Address on Device Display Panel

Specify whether to display the device IP address on its control panel.

Note

- The IP address display position or order on the control panel varies depending on the device model.
- This is displayed only if/when supported by the machine.

### Media Slot Use

Specify whether or not to allow users to use the machine's media slot.

Note

- This is displayed only if/when supported by the machine.

#### Store to Memory Device

Specify whether or not to allow users to store the scanned data to a USB flash memory device or an SD card using the media slot.

#### Print from Memory Storage Device

Specify whether or not to allow users to print the data from a USB flash memory device or an SD card using the media slot.

### Compatible ID

You can enable or disable the Compatible ID setting.

### PDF File Type: PDF/A Fixed

Converts all PDF files generated in the machine to PDF/A files.

Note

- A PDF/A file cannot be opened in a version earlier than Acrobat 4.

### Stapleless Stapler Settings

Specify the stapleless stapler settings.

#### Erase Margin for Stapleless Stapler

The staple may come off easily if the stapleless stapler is applied to an image printed in a stapling position.
Using this function enables you to remove the image printed in the stapling position and prevent the staple from coming off. Alternatively, you can change the position of the binding margins so that stapling is not directly applied to the image.

Note

- Depending on printing functions, the margin adjustment method will vary.
  - When using printer driver, adjust the margins on the application you use.
  - When using the Document Server and copier functions from the operation panel of the device, adjust the margins on the operation panel.
  - When using Document Server from Web Image Monitor, adjust margins on the Edit page.
- If you use this function, the output may differ from the thumbnail image on Document Server.

#### Stapling Method for Stapleless Stapler

Specify a stapling method for stapleless stapler.

#### Single

Applies single stapling. The stapling time is shorter than Double.

#### Double

Applies double stapling. This method is stronger than Single.

#### Auto Switch Staple/Stapleless Stapler

Specify whether or not to switch between regular and stapleless stapling modes automatically.
If On is selected, stapleless stapling is applied to a document of less than six sheets, or regular stapling to six sheets or more.

### Remote Main Power On

Specify whether or not to enable the Remote Main Power On function.
This function allows you to turn on the main power of the machine remotely by sending the Wake-on-LAN (WOL) packet.

### Prohibit printing stored files from Web Image Monitor

Specify whether or not to allow users to print stored files from Web Image Monitor.

Note

- The Print button may not appear if Prohibit is set for Prohibit printing stored files from Web Image Monitor on the following pages:
  - Document Server (Shared Folder/Individual Folder)
  - Fax Received File
  - Print Job List

### Energy Saving Recovery for Business Application

If only applications which run without the machine (printer/copier/scanner functions) are used, selecting On (Energy Saving) will reduce power consumption. In this mode, it will take time for the machine to return to the normal mode.

### Silent Mode

Specify whether or not to use silent mode.
Selecting On reduces the operation sound by printing and scanning originals slowly.

### Ready State After Printing

You can specify the state of the printer when printing documents during Sleep Mode.
Selecting Control Panel On changes the printer mode to standby after printing.
Selecting Cntrl Panel Off (EnSvg) returns the printer to Sleep Mode after printing.

### Human Detection Sensor

Specify whether or not to enable the human detection sensor.
If Active is selected, the machine detects a user's presence nearby and exits power saving mode, so that the machine's control panel will be ready to use in a short time.

### Energy Saving Recovery for Business Application

If only applications which run without the machine (printer/copier/scanner functions) are used, selecting On (Energy Saving) will reduce power consumption. In this mode, it will take time for the machine to return to the normal mode.

### ADF Operation: Copier/Document Server

Select either of the following when using the copier or document server.

#### Silent Mode

Reduces the operation sound by scanning originals slowly.

#### Productive Mode

Gives priority to the scanning speed.

### Shift to Main Power-Off When Network Disconnected

Set whether to turn the main power off when the network is disconnected.

### Screen display function when network is not connected

Set whether to enable or disable the function to display a screen when a network connection error occurs.

### Output Priority When Paper is Fed to Finisher

Specify the output mode when ejecting paper from a finisher.
It may take more time to exit power saving mode if a finisher is installed.

#### Print Start Time

Exits power saving mode faster. However, print speed is reduced.

#### Continuous Print Speed

Gives priority to print speed. It takes more time to return to normal mode than Print Start Time.

### Allow Log Collection

Set whether to allow or deny log acquisition via @Remote.

### Ability to log out while scanning

Set whether to enable or disable the logout function while scanning a copy.

## Output Tray

Select the output tray for each function.

Note

- Available output trays depend on machine type or options installed.
- The output tray selection for individual functions does not appear if the machine has only one tray installed.

### Copier

Select the output tray you want to use for the copier function.

### Fax

Select the output tray you want to use for the fax function.

### Printer

Select the output tray you want to use for the printer function.

### Document Server

Select the output tray you want to use for the Document Server function.

## Paper Tray Priority

Select the priority tray for each function.
Paper Tray Priority is the tray selected immediately after the printer is turned on, and when Auto Select is chosen as the paper source in a job.

Note

- Available input trays depend on machine type or options installed.

### Copier

Select the priority tray you want to use for the copier function.

### Fax

Select the priority tray you want to use for the fax function.

### Printer

Select the priority tray you want to use for the printer function.

## Cover Sheet Tray

Cover Sheet Tray is displayed only if the machine has a cover sheet function.

### Tray to set

Specify whether or not to set the cover sheet tray.
When setting the cover sheet tray, first select the paper tray you want to use for cover sheet.

Note

- Available paper trays depend on machine type or options installed.
- When None is selected in the Tray to set list, settings configured for Apply Duplex and Display Time are disabled.

### Apply Duplex

Specify whether or not to use the tray for duplex printing.
Even if On is selected, the tray may not be suitable for duplex printing, depending on the type and thickness of the paper that is loaded in it.

Note

- This setting is enabled only when At Mode Selected is selected for Display Time. If Full Time is selected for Display Time, the setting in Apply Duplex on the Configuration: Device Settings: Paper page is used.

### Display Time

Select when the cover sheet tray should be shown in the copy function screen on the machine's control panel.

#### At Mode Selected

The cover sheet indication appears on the tray item when the cover sheet function is selected.

#### Full Time

The cover sheet tray indication always appears on the tray item.

## Slip Sheet Tray

Slip Sheet Tray is displayed only if the machine has a slip sheet function.

### Tray to set

Specify whether to set the slip sheet tray.
When setting the slip sheet tray, first select the paper tray you want to use for slip sheet.

Note

- Available paper trays depend on machine type or options installed.
- When None is selected in the Tray to set list, settings configured for Apply Duplex and Display Time are disabled.

### Apply Duplex

Specify whether to use the tray for duplex printing.
Even if On is selected, the tray may not be suitable for duplex printing, depending on the type and thickness of the paper that is loaded in it.

Note

- This setting is enabled only when At Mode Selected is selected for Display Time. If Full Time is selected for Display Time, the setting in Apply Duplex on the Configuration: Device Settings: Paper page is used.

### Display Time

Select when the slip sheet tray should be shown in the copy function screen on the machine's control panel.

#### At Mode Selected

The slip sheet indication appears on the tray item when the slip sheet function is selected.

#### Full Time

The slip sheet tray indication always appears on the tray item.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##