# SYSLOG Transfer Setting
Device Management > Configuration > Device Settings > SYSLOG Transfer Setting

Use this page to configure the settings for SYSLOG.

Note

- Settings on this page can be changed by the following administrators and users:
  - Machine Administrator
  - Login users
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.

### Transfer to SYSLOG Server

Enable or disable the function that transfers recorded logs to the SYSLOG server.

### SYSLOG Destination

Displays the setting items related to the SYSLOG destination.

#### Address

Specify the address of the SYSLOG destination.

#### Port Number

Enter the port number of the SYSLOG destination. Enter a value between 1 and 65535. The default value is 6514.

### Verification of SYSLOG Server Certificate

Enable or disable verification of the SYSLOG server certificate.

### Upload Certificate

Displays whether the SYSLOG server certificate has been installed.

#### Execution

Displays the Upload screen for the SYSLOG server certificate.

For details about the Upload of SYSLOG Server Certificate page

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##