# Remote Panel Operation
Device Management > Remote Panel Operation

Monitor the device's screen/Operate the device remotely.

### Language

Change the language of the monitoring/operation window.

### Panel Control

#### Remote Operation

Remote Panel Operation can be enabled or disabled.

#### Lock the Machine’s Panel

Locking the screen prevents any operation from the device's touch panel.

#### Hide the Machine’s Panel

Darken the device's screen to hide any operations being carried out through Remote Panel Operation.

### Settings

#### Display Size

Select the display size of the device's screen.

#### Display Mode

Quality: Priority is given to screen quality/ Speed: Priority is given to speed.

### Exit

Finish monitoring/remote operation.

Note

- This function can only be used by the ‘Machine Administrator’.
- This function must be enabled in the settings before it can be used. Go to "User Tools">"Basic Settings for Extended Devices">"Remote Panel Operation">"Remote Operation/Monitoring Functions".
- During Remote Panel Operation, priority is given to remote operation and monitoring, so the device will not automatically transition to Energy Saving Mode. Also, ‘Auto Logout’ and ‘System Auto Reset’ will not work.
- If Remote Panel Operation is attempted while the device is being used, a dialog box will be displayed on the device to request permission for Remote Panel Operation to go ahead.
  If more than 180 seconds have passed since the device was last used, Remote Panel Operation will go ahead without displaying the permission dialog.

##