# Timer
Device Management > Configuration > Device Settings > Timer

Configure settings to control the functions supported by the machine.

Note

- Settings on this page can be changed by the following administrators and users:
  - Machine Administrator
  - Login users (all items), if:
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.
- Some items may not appear depending on machine type or configuration.

### Sleep Mode Timer

The sleep mode timer automatically turns off the device when it is left idle for a specified period.
Enter the time period that the device must be idle before switching to sleep mode. Enter a value between 1 and 60 (minutes). Depending on machine type, enter a value between 1 and 240 (minutes).

### System Auto Reset Timer

Specify whether to reset the device to its initial status (as when the device was first turned on), when left idle for a specified period.
If you select On, you must then enter the time before reset to the initial status. Enter a value between 10 and 999 (seconds).
If you select Off, device settings remain unchanged until the device is turned off.

### Copier/Document Server Auto Reset Timer

Specify whether to reset the copier/document server settings to their initial status (as when first turned on), when the copier/document server functions are left idle for a specified period.
If you select On, you must then enter the time before reset to initial status. Enter a value between 10 and 999 (seconds).
If you select Off, device settings remain until turned off.

### Fax Auto Reset Timer

Specify the time before resetting the device's fax settings to their initial status (as when first turned on) when the fax function is idle for a specified period.
If you select On, you must then enter the time before reset to initial status. Enter a value between 30 and 999 (seconds).
If you select Off, device settings remain until turned off.

Note

- If the cloud fax function is enabled, this function will not be available.

### Scanner Auto Reset Timer

Specify whether to reset the device's scanner settings to their initial status (as when first turned on), when the scanner function is idle for a specified period.
If you select On, you must then enter the time before reset to initial status. Enter a value between 10 and 999 (seconds).
If you select Off, device settings remain until turned off.

### Printer Auto Reset Timer

Specify whether to reset the device's printer settings to their initial status (as when first turned on), when the printer function is idle for a specified period.
If you select On, you must then enter the time before reset to initial status. Enter a value between 10 and 999 (seconds).
If you select Off, device settings remain until turned off.

### Auto Logout Timer

Select this to automatically log out the login user from the control panel if he/she does not use the machine for a specified period.
If you select On, you must then enter the time period that elapses before the user is automatically logged out. Enter seconds between 10 and 999 (seconds).
If you select Off, the user remains logged in until he/she manually logs out.

### Fusing Unit Off Mode On/Off

This function automatically turns the fusing unit's heater off when the device is left idle for a specified period.
Specify whether or not to put the device into fusing unit off mode.

Note

- If you select On, Low Power Mode Timer will be unavailable.

#### Fusing Unit Off Mode Timer

Specify how long the device waits before it goes into fusing unit off mode.

#### Exit Fusing Unit Off Mode

Specify when to exit the fusing unit off mode.

#### On Printing

Exits the fusing unit off mode when a print job is processed.

#### On Operating Control Panel

Exits the fusing unit off mode when you switch from one function to another function on the machine's control panel.

## Weekly Timer

Configure the weekly timer.
The weekly timer automatically puts the device into sleep mode and turns the main power off as specified.
If you select Active (Daily), select the Active check boxes, and then specify a timer type and enter the time.
If you select Active (Day of the Week), select the Active check boxes, and then specify a timer type and enter the time on the specified day of the week.
For example, to put the device into sleep mode when lunchtime begins (12:00) and turn the main power off during nighttime (18:00-09:00 next morning), use the following settings:

Setting Item | Setting Value
--- | ---
Weekly Timer | Active (Daily)
Main Power On | 09:00 (Workday begins)
Enter Sleep Mode | 12:00 (Lunchtime begins)
Main Power Off | 18:00 (Workday ends)

The device will remain in sleep mode unless an operation is performed after sleep mode.
If the Weekly Timer Code setting is configured, the device will not exit sleep mode or receive jobs until you enter the weekly timer code on the control panel of the machine. But you can select Cancel Weekly Timer Code for the timer type and enter the time to make the machine exit sleep mode and operate jobs after the specified time.
If you want to turn the main power off all day on Saturdays and Sundays only, select Active (Day of the Week), and then specify the schedule for each day.

Note

- You can enter a time between 0:00 and 23:59.
- If you want to give priority to the first print speed during work hours, do not configure settings to enable sleep mode.

### Main Power On Timer Suspension Period

Specify whether or not to suspend the weekly timer in the specified period.
If you select Active, the machine will ignore the Main Power On time in the specified period.
Once the main power is turned off in timer suspension period, it remains off because the machine ignores the Main Power On time. When the specified period is over, the weekly timer restarts. This function is useful when you want to suspend the weekly timer and turn the main power off only for the specified period of time such as summer and winter vacations.

### Weekly Timer Code

Specify whether or not to request a weekly timer code for manual power on or exit from sleep mode.
When On is selected, enter the weekly timer code. Enter a value between 0 and 99999999.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##