# Scan Settings
Device Management > Configuration > Scanner > Scan Settings

Configure the default settings used for scanning originals.

Note

- Settings on this page can be changed by the following administrators and users:
  - Machine Administrator
  - Users logged in to a device that is set to perform user authentication
    Users must have normal scanner operation rights and permission to change settings that usually only administrators can change.

### A.C.S. Sensitivity Level

Sets the sensitivity level for detecting color/black and white when scanning originals.

### Wait Time for Next Original(s)

#### Exposure Glass

To divide originals and scan them separately into a single file using the exposure glass, specify Continuous Wait, Off, or Set Wait Time for the waiting status.

#### Continuous Wait

The machine will wait for additional originals until the # key is pressed. Scanning begins as soon as any additional originals are placed and the start key is pressed. You can end scanning and begin sending by pressing the # key.

#### Off

The machine does not wait for additional originals and begins sending as soon as each original is scanned.

#### Set Wait Time

Using the number keys, specify the time (3 to 999 seconds) that the machine waits for additional originals. Scanning begins as soon as any additional originals are placed and the start key is pressed. During this time, you can end scanning and begin sending by pressing the # key. When the specified time elapses, the scanned files are automatically sent.

#### SADF

To divide originals and scan them separately into a single file using the ADF, specify Set Wait Time or Continuous Wait for the waiting status.

Note

- This setting is available only on machines that are equipped with the Auto Document Feeder.

#### Continuous Wait

The machine will wait for additional originals until the # key is pressed. Scanning begins as soon as any additional originals are placed and the start key is pressed. You can end scanning and begin sending by pressing the # key.

#### Set Wait Time

Using the number keys, specify the time (3 to 999 seconds) that the machine waits for additional originals. Scanning begins automatically if additional originals are placed within this time. During this time, you can end scanning and begin sending by pressing the # key. When the specified time elapses, the scanned files are automatically sent.

### Background Density of ADS (Full Color)

Adjusting the background density can reduce excessive grayness and shading, which can appear on scans if the original is a newspaper or other semi-transparent media.

### Blank Page Detect

Specify whether or not to display a warning message if the original is a blank sheet.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##