=====================================================================
License Agreement for Fuji Xerox PCL Mini Driver
=====================================================================

1. PROPRIETARY RIGHTS: Title, ownership rights, and intellectual
   property rights in the SOFTWARE shall remain in Fuji Xerox and
   its third party suppliers.  You have no rights in the SOFTWARE
   except as expressly granted in accordance with this agreement.
   
2. LICENSE:  Under this agreement, you are granted a non-exclusive
   license to use the SOFTWARE for the purpose of using with
   compatible Fuji Xerox products in Japan.  You are not permitted to
   (1) assign, sublicense, sell, rent, lease, convey, or transfer the
   SOFTWARE to any third party by any tangible media such as floppy
   disk, magnetic tape, or CD-ROM, (2) distribute the SOFTWARE on a 
   network or by a telephone line available to the public or (3) 
   alter, modify, decompile, disassemble, reverse engineer, or create
   derivative works based on the whole or any part of the SOFTWARE.
   If any direction on usage or restriction for the SOFTWARE is 
   expressly specified in this web site, you are required to follow
   such direction.
   
3. TERM: This agreement is effective upon installing the SOFTWARE
   until you terminate the agreement by destroying the SOFTWARE. 
   This agreement will also terminate if you fail to abide by any 
   terms of this agreement.  In case of termination, you must
   promptly destroy the SOFTWARE.
   
4. LIMITED WARRANTIES: THE SOFTWARE IS SUPPLIED STRICTLY ON AN
   'AS IS' BASIS WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESSED OR
   IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY OF
   MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE, WITH RESPECT
   TO THE SOFTWARE. YOU ARE RESPONSIBLE FOR CHOOSING, MAINTAINING AND
   MATCHING OTHER HARDWARE AND SOFTWARE COMPONENTS IN COMBINATION OF
   THE SOFTWARE.  IN NO EVENT, SHALL FUJI XEROX, FUJI XEROX CHANNEL
   PARTNERS, AUTHORIZED DEALERS AND THEIR THIRD PARTY SUPPLIERS BE
   LIABLE FOR ANY LOSS OR DAMAGE INCLUDING INCIDENTAL OR
   CONSEQUENTIAL LOSS OR DAMAGE, ARISING FROM USE OF OR INABILITY TO
   USE SOFTWARE, OR ANY MODIFICATION OF THE SOFTWARE.
   
5. EXPORT CONTROL: You are not allowed to export the SOFTWARE in part
   or whole, directly or indirectly, in violation of any 
   restrictions, laws or regulations imposed by the government of
   Japan or any other relevant countries, and are required to obtain
   necessary approval prior to exporting the SOFTWARE.
   
=====================================================================
Fuji Xerox PCL Mini Driver

 Microsoft(R) Windows(R) XP Professional x64 Edition
 Microsoft(R) Windows Server(R) 2003 x64 Editions
 Microsoft(R) Windows Vista(R) x64 Editions
 Microsoft(R) Windows Server(R) 2008 x64 Editions
 Microsoft(R) Windows(R) 7 x64 Editions
 Microsoft(R) Windows Server(R) 2008 R2
 Microsoft(R) Windows(R) 8 x64 Editions
 Microsoft(R) Windows Server(R) 2012

GPD version 1.1.1
=====================================================================

This document provides information about the print driver on the 
following items: 
1. Prerequisites
2. Model Names
3. File Configuration
4. Installation
5. Version Improvements
6. Limitations
7. Checking the driver version
8. Inquiries


----------------
1. Prerequisites
----------------
Please note that this print driver operates on a computer with 
an AMD64-based microprocessor or an Intel Extended Memory 64Technology-based
microprocessor (Intel EM64T and above) and an upward-compatible processor, running
Microsoft(R) Windows(R) XP Professional x64 Edition
Microsoft(R) Windows Server(R) 2003 x64 Editions
Microsoft(R) Windows Vista(R) x64 Editions
Microsoft(R) Windows Server(R) 2008 x64 Editions
Microsoft(R) Windows(R) 7 x64 Editions
Microsoft(R) Windows Server(R) 2008 R2
Microsoft(R) Windows(R) 8 x64 Editions
Microsoft(R) Windows Server(R) 2012
(For clock speed of the CPU and memory, make sure that the system 
 configuration is recommended by the operating system.)  


--------------
2. Model Names
--------------
Supported model names of the driver and names that appear during
installation are as follows: 

Model Name                  : Model name that appear during installation

ApeosPort 550 I             : FX AP 550 I PCL
ApeosPort 450 I             : FX AP 450 I PCL
ApeosPort 350 I             : FX AP 350 I PCL
DocuCentre 550 I            : FX DC 550 I PCL
DocuCentre 450 I            : FX DC 450 I PCL

---------------------
3. File Configuration
---------------------
FXUCCM01.INF
FXUCCM01.INI
FXUCCM01.GPD
FXUCNS01.GPD
FXUCNS02.GPD
FXUCNS03.GPD
FXUCNS04.GPD
FXUCNS05.GPD
FXUCU001.dll
FXUCNS01.CAT

---------------
4. Installation
---------------
You can install this driver by downloading from our web site.
These methods of installation are described below.  

Important
----------
* Close all the running applications before installing the print 
  driver.  
* Always reboot the computer after installing an upgraded version of 
  the print driver.  
* If you have deleted an older version of the print driver, always 
  reboot the computer before installing the new version.  
* The installation procedures are written with the assumption that
  standard settings have been configured in Windows.
  The procedures may differ if the start menu or folder options have
  been changed.
* You may not be able to install correctly if installation is made using 
  Power User rights. Re-install as an Administrator. 
* Installation may not be successful if this driver is not installed
  using the following procedure.
* Please refer to the following section of this chapter for driver
  deletion method under Windows Vista, Windows Server 2008, Windows 7,
  Windows Server 2008 R2, Windows 8, and Windows Server 2012.
   * About driver deletion method (When using Windows Vista,
     Windows Server 2008, Windows 7, Windows Server 2008 R2,
     Windows 8, or Windows Server 2012)
* Please refer to the following section of this chapter for installation
   method using plug-and-play under Windows 7, Windows Server 2008 R2,
   Windows 8, and Windows Server 2012.
   * About driver installation method using plug-and-play
     (When using Windows 7, Windows Server 2008 R2, Windows 8, or
      Windows Server 2012)

*** Installation from downloaded data via the web site
You can download the latest driver from our web site.  
Refer to "8. Inquiries" for our web site address (URL).  
Communication charges will be borne by the customer.  

1) Double-click the downloaded compressed file (.exe format) to 
   decompress.  
2) Activate the "Add Printer Wizard".    
   2a) For Windows XP, click the "Start" button.  Point to
       "Settings" and click "Printers and Faxes".  
       Click the "Add a printer" icon.  
   2b) For Windows Server 2003, click the "Start" button.  Point to 
       "Settings" and click "Printers and Faxes".  
       Double-click the "Add Printer" icon.  
   2c) The following steps are available for use when installing printer 
       under Windows Vista.
       * Click "Start" button and then click "Control Panel".
       * Select "Printers and Faxes" in "Hardware and Sound"
          and then select "Add a Printer".
   2d) On Windows Server 2008, select menu in the order below from
       the "Start" button.
       Go to "Start" > "Control Panel" > "Printers".
       Select "File" > "Run as Administrator" > "Add Printer" on the menu.
   2e) The following steps are available for use when installing 
        printer under Windows 7 or Windows Server 2008 R2.
       * Click "Start" button and then click "Devices and Printers".
       * Select "Add a printer" in "Devices and Printers".
   2f) The following steps are available for use when installing 
        printer under Windows 8 or Windows Server 2012.
       * Go to "Control Panel" > "Hardware and Sound" > "Devices and Printers".
       * Select "Add a printer" in "Devices and Printers".
3) Specify the printer connection.  
   * For a local printer:  
     Specify the local printer going through the menu displayed on Windows. 
     Proceed to step 4).  
   * For a network printer:
     Specify the desired printer from the network going through the menu
     displayed on Windows.
     Contact the network administrator if you have any queries.
     If other printers are installed, a message asking whether
     to set this as the default printer is shown.  Click "Yes"
     if you want to set it as a default printer.  
     Proceed to step 11).  
4) Specify the printer port.  
   Create a port if there is no output port.
   Please refer to the "Frequently Asked Questions" from our driver 
   download page for the port creation method. 
   For our URL web page, please refer to "5. Inquiries".
5) Click "Have Disk" from the "Add Printer Wizard" screen.  
   An "Install From Disk" screen is displayed.  
   Specify the directory containing the uncompressed files in step 1)
   in the "Copy manufacturer's files from" box. Click "OK".  
6) A list of printers is displayed. Select the desired printer.  
   If the selected printer is already installed, a message asking 
   whether to replace the existing driver is displayed.  
   When installing a new version of the print driver, select 
   "Replace existing driver" or "Replace the current driver".
   The older version of the driver cannot be deleted if it is used 
   in an application.  In this case, close the application. 
7) A dialog box for specifying the printer name is displayed.  
   To change the printer name, enter any name in the "Printer name" 
   box.  
   If other printers are installed, a message asking whether to set 
   this as the default printer is shown.  
   7a) When using Windows XP,Windows Server 2003, 
       please click "Yes" button if you want to set a printer as default.
   7b) When using Windows Vista, Windows Server 2008, Windows 7,
       Windows Server 2008 R2, Windows 8, or Windows Server 2012, please check
       the "Set as the default printer" checkbox if you want to set a printer
       as default. 
           As the following steps are slightly different for Windows Vista,
           Windows Server 2008, Windows 7, Windows Server 2008 R2, Windows 8,
           and Windows Server 2012, please proceed to step 13).
8) Specify whether to share this printer with other network users.  
9) A dialog box specifying whether to print the test page after 
   installation is shown. Load A4 paper to the printer, select "Yes" and
   then "Next". Select "No" and click "Next" if you do not wish to print the 
   test page.
10) A dialog box to confirm the settings is displayed.  Click 
    "Finish" after confirming the settings.  
11) A dialog box to confirm the continuation of installation may be displayed.  
    If the dialog box is not displayed, go to the next step.
    For Windows XP and Windows Server 2003, a message saying
         that it did not pass the Windows Logo Test will be displayed
         but this does not cause functional problem.
         Click "Continue Anyway".  
12) The necessary files are copied and a new printer icon is 
    created.  
    If you have printed the test page, a printer test result 
    confirmation message is displayed. 
    By the above steps, the driver installation is completed. Please 
    proceed to step 17).
13) For Windows Vista, Windows Server 2008, Windows 7, Windows Server 2008 R2, 
    Windows 8, and Windows Server 2012, this is the start of the driver
    installation.
    * The installation confirmation screen published by Fuji Xerox Co., Ltd.
      may be displayed, but it is not a functional problem.
      Click "Install".
    * You can continue with the installation in the "User Account Control"
      dialog box.
    Click the "Continue" button to proceed. For users without 
    administrator rights who wish to install the driver, 
    select the option of user with administrator rights,
    enter the password and then click "OK". 
    "User Account Control" dialog is not displayed when the driver is 
    installed through "Run as Administrator".
14) Please ignore the pop-up dialogue of "Windows can't verify 
    the publisher of this software" if it appears.  When you find the dialog, 
    click "Install this driver software anyway." to continue with
    the installation.
       * A message "Windows can't verify the publisher of this driver software"
         appears depending on the version of Windows.
15) Make sharing settings.  
    If the driver is installed with administrator rights, a dialog to make 
    sharing settings appears.  Make sharing settings in this dialog and 
    click "Next".  
16) The driver installation is completed.
    Click "Print a test page" button if you want to print a test page. 
    Please refer to step 9) for the details of test page printing.

    Next, we set the installed printer options.  
17) Click the printer icon.  
18) From the "Printer" menu, click "Properties".  
19) Click the "Options" tab.  
    Perform the setting when the "Options" tab is displayed.   

About driver deletion method 
(When using Windows Vista, Windows Server 2008, Windows 7,
Windows Server 2008 R2, Windows 8, or Windows Server 2012)
-----------------------------------------------------------
To remove drivers from system completely, please delete drivers and driver
package going through the following steps.
Please note that driver package can not be deleted by executing driver 
uninstall tool.

  <<Windows Vista, Windows Server 2008>>
   * Click "Start" and open "Control Panel", then select "Printer" in
     "Hardware and Sound" panel.
   * Delete printer icon in "Printers" folder.
   * Right-click in "Printers" folder and select "Run as 
     Administrator".
     Click "Server Properties" then "Printer Server Properties" 
     window is displayed.
   * Select the driver to be deleted from the "Driver" tab and click 
     "Remove" button.
   * Select "Remove driver and driver package.", then click "OK" 
     button.
   * When the driver is in use, a message appears and the driver package
     may not be able to be deleted.  In such case, reboot the computer and 
     try to delete again.   
   * Restart the computer.

  <<Windows 7, Windows Server 2008 R2, Windows 8, Windows Server 2012>>
  <<Windows 7, Windows Server 2008 R2>>
  * Click "Start" and select "Devices and Printers".
  <<Windows 8, Windows Server 2012>>
  * Go to "Control Panel" > "Hardware and Sound" and select "Devices and 
    Printers".
  * Click the printer icon in the "Devices and Printers" folder, 
    and select "Remove device" menu to delete it.   
  * Click any of the icons displayed in "Printers and Faxes" in the
    "Devices and Printers" folder and select "Print server properties".  
  * Click the "Drivers" tab to open it.  
  * When the "Change Driver Settings" button is displayed, click it.  
  * Select a driver to delete from the "Drivers" tab and click the "Remove" 
    button.  
  * Select "Remove driver and driver package" and click the "OK" button.  
  * When the driver is in use, a message appears and the driver package
    may not be able to be deleted.  In such case, reboot the computer and 
    try to delete again.   
  * Restart the computer.

About driver installation method using plug-and-play
(When using Windows 7, Windows Server 2008 R2, Windows 8, or 
Windows Server 2012)
-------------------------------------------------------------
When a driver is installed using plug-and-play, it may not
be installed properly.  In such case, follow the steps below to reinstall
the driver.

  * Select "Devices and Printers".
  * In the "Devices and Printers" folder, right-click the icon of this
    printer and select "Properties". 
    *When the icon is disabled and inoperable, turn off/on the printer
     and make sure that the printer is connected securely with a cable. 
  * Select this printer in "Device Functions" in the "Hardware" tab, and
    click the "Properties" button to open the Properties dialog. 
  * Click the "Change settings" button and open a new "Properties" dialog.  
  * In the new "Properties" dialog, open the "Driver" tab, and click the 
    "Update driver" button to open the "Update driver software" dialog.  
  * Select "Browse my computer for driver software" and specify 
    the driver's location under "Search for driver software in this location:".
    Click "Next".
    *Please refer to the steps for driver installation using "Add Printer 
    Wizard" for how to prepare the driver.   
  * When a message stating that the driver has been updated successfully,  
     click "Close" to close the dialog.  
     Now, the driver has been reinstalled successfully.  


-----------------------
5. Version Improvements
-----------------------
This section describes the modifications made for each upgraded 
version.

[Ver.1.1]
* Vista OS support
* Unsupported function corrected
* Server 2008 OS support
* 7 OS support

[Improvements from Ver 1.1]
* Supported Microsoft(R) Windows(R) 8, Microsoft(R) Windows Server(R) 2012.


--------------
6. Limitations
--------------

===========================
Driver-Specific Limitations
===========================

* This driver provides the basic print functions based on the 
  prerequisites in 1). Please note that it is not guaranteed 
  that the functionality of this print driver and its functional 
  compatibility on 32-bit OS environment is the same 
  as the print driver in the past.
  
* If a B/W document is printed on a color printer, please set the 
  print driver setting to B/W. If printing is performed using 
  color setting, it will be counted as a color print.

* When printing an odd-page document in duplex, a blank page may be 
  added to the last page of the document depending on the 
  operating system (thereafter OS). In this case, display the 
  properties dialog box from the printer icon and uncheck 
  the "Enable advanced printing features" check box on the 
  "Advanced" tab. However, note that reverse order printing and 
  booklet printing will be unavailable when this check box is 
  unchecked. 
  Depending on the application used by the customer, blank pages for 
  page adjustment will be inserted automatically according to 
  the conditions like the number of copies specified regardless of 
  the type of OS. This operation cannot be prevented as it is 
  part of the specification of the application. The blank inserts 
  by the OS or application will be counted. 

* This driver does not support the authentication function. As a 
  result, printing is unavailable if authentication is required from 
  the printer.

* This driver does not support User ID function. Therefore, counting
  of print jobs is unavailable using DocuHouse.

* Application prints such as secure print, save to mailbox , delay 
  print are not supported. 
  
* Direct FAX function is not supported. 

* If this print driver is used in a shared printer, it is necessary 
  to make sure that this mini driver is operating on both the server and 
  client. 
  
* It is necessary that the client using the shared printer fulfill 
  the prerequisite of 1. (It cannot be operated on 32-bit OS.)

* This print driver does not support Citrix MetaFrame(R).

* Printing may not be available using this print driver depending on 
  the memory capacity of the printer. If the printing resolution 
  drops and the page count are huge, you can try to print the 
  document by subsets or increase the memory quota of the 
  printer. 
  
* This print driver will take a longer processing time compared to 
  the 32-bit full function print driver. 


------------------------------
7. Checking the driver version
------------------------------
You can check the driver version using the following method.

* GPD Version
1) Select the printer icon and click "Properties" from the "File" 
   menu. 
2) Move to "Advanced" tab and right click on "**** Advanced" 
   (The printer icon name will be displayed at ****).  
   Click "About". 
3) The "About" dialog box will be displayed. 
   Confirm the "GPD version".


------------
8. Inquiries
------------
    The latest software is available on our web site.

        http://www.fxap.com.sg/default.jsp

    Communication charges will be borne by the customer.
