===============================================================================
License Agreement
===============================================================================

1. PROPRIETARY RIGHTS: Title, ownership rights, and intellectual
   property rights in the SOFTWARE shall remain in Fuji Xerox and
   its third party suppliers. You have no rights in the SOFTWARE
   except as expressly granted in accordance with this agreement.

2. LICENSE:  Under this agreement, you are granted a non-exclusive
   license to use the SOFTWARE for the purpose of using with
   compatible Fuji Xerox products in Japan. You are not permitted to
   (1) assign, sublicense, sell, rent, lease, convey, or transfer the
   SOFTWARE to any third party by any tangible media such as floppy
   disk, magnetic tape, or CD-ROM, (2) distribute the SOFTWARE on a
   network or by a telephone line available to the public or (3)
   alter, modify, decompile, disassemble, reverse engineer, or create
   derivative works based on the whole or any part of the SOFTWARE.
   If any direction on usage or restriction for the SOFTWARE is
   expressly specified in this web site, you are required to follow
   such direction.

3. TERM: This agreement is effective upon installing the SOFTWARE
   until you terminate the agreement by destroying the SOFTWARE.
   This agreement will also terminate if you fail to abide by any
   terms of this agreement. In case of termination, you must
   promptly destroy the SOFTWARE.

4. LIMITED WARRANTIES: THE SOFTWARE IS SUPPLIED STRICTLY ON AN
   'AS IS' BASIS WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESSED OR
   IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY OF
   MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE, WITH RESPECT
   TO THE SOFTWARE. YOU ARE RESPONSIBLE FOR CHOOSING, MAINTAINING AND
   MATCHING OTHER HARDWARE AND SOFTWARE COMPONENTS IN COMBINATION OF
   THE SOFTWARE. IN NO EVENT, SHALL FUJI XEROX, FUJI XEROX CHANNEL
   PARTNERS, AUTHORIZED DEALERS AND THEIR THIRD PARTY SUPPLIERS BE
   LIABLE FOR ANY LOSS OR DAMAGE INCLUDING INCIDENTAL OR
   CONSEQUENTIAL LOSS OR DAMAGE, ARISING FROM USE OF OR INABILITY TO
   USE SOFTWARE, OR ANY MODIFICATION OF THE SOFTWARE.

5. EXPORT CONTROL: You are not allowed to export the SOFTWARE in part
   or whole, directly or indirectly, in violation of any
   restrictions, laws or regulations imposed by the government of
   Japan or any other relevant countries, and are required to obtain
   necessary approval prior to exporting the SOFTWARE.

===============================================================================
ART EX Print/Direct Fax Driver Ver.2.7.16 Additional Information
===============================================================================

This document provides information about the driver on the
following items:

1. Target Hardware Products
2. Requirements
3. Installation
4. Version Improvements
5. Limitations
6. Inquiries

---------------------------------------------------
1. Target Hardware Products
---------------------------------------------------
FUJI XEROX ApeosPort-III C3305
           ApeosPort-III C2205
           DocuCentre-III C3305
           DocuCentre-III C2205

---------------------------------------------------
2. Requirements
---------------------------------------------------
1. Please note that this print/direct fax driver operates on a computer running on 
   the following operating system. 

    Microsoft(R) Windows(R) 2000
    Microsoft(R) Windows(R) XP
    Microsoft(R) Windows Server(R) 2003
    Microsoft(R) Windows Vista(R)
    Microsoft(R) Windows Server(R) 2008
    Microsoft(R) Windows(R) 7
    Microsoft(R) Windows(R) 8
    Microsoft(R) Windows(R) 8.1
    Microsoft(R) Windows(R) 10

  Click the following URL to see the latest update on OS support.
  http://www.fujixerox.co.jp/download/defacto/

2. This print/direct fax driver works correctly with the combinations of the 
   below mentioned printer software versions.

    * ApeosPort-III C3305 	Controller ROM Version 1.0.0 or later
    * ApeosPort-III C2205 	Controller ROM Version 1.0.0 or later
    * DocuCentre-III C3305	Controller ROM Version 1.0.0 or later
    * DocuCentre-III C2205	Controller ROM Version 1.0.0 or later

---------------------------------------------------
3. Installation
---------------------------------------------------
Click the following URL to know how to install this driver.
http://www.fujixerox.co.jp/download/info/manual_inst.html

---------------------------------------------------
4. Version Improvements
---------------------------------------------------
[Improvements from Ver 2.7.1]
* Added [IP Fax (SIP)] feature to the direct fax driver.
  Also, the design of the sending sheet has changed due to the new feature.
  Added [Dear] to the selection options of the [Name] combo box.
  Added [Mr.] to the selection options of the [Affiliation] combo box.
* Fixed the bug of a possible failure to correctly retrieve message source information 
  from the application that used PSLAD2, made by ACEL, Inc.
* Fixed the problem that the options were displayed with wrong names in "Image Shift".

[Improvements from Ver 2.7.3]
* Supported Windows(R) 7.
* Fixed the problem that the settings of "User Details Setup" would be initialized
  when a user logged in again using a session printer in the Citrix Presentation Server(TM)
  and XenApp(TM) environment.
* Fixed the problem that an error would occur when printing started from a certain
  multithread application
* Fixed the problem that an error would occur when a printer was installed in the
  environment of using a printer with an alternative driver added.
* Fixed the problem that collated output was not performed when the hard disk is
  not installed.

[Improvements from Ver 2.7.7]
* Fixed the problem that a printing error may occur when documents with an image 
  included are output from a certain application.
* Alleviated the problem of application errors occuring when printing from specific
  applications after the direct fax driver has been updated.

[Improvements from Ver 2.7.10]
* Fixed the bug of a possible error when accessing the driver from an external tool.

[Improvements from Ver 2.7.13]
* Fixed the problem that a certain printing pattern may not be performed normally 
  through a certain application.
* Added functional restrictions to some functions to respond to the problem that 
  a setting value is not reflected on the output in the situation where Internet Explorer 
  in Protection mode is running.
  Please refer to "5. Limitations" for more details.

[Improvements from Ver 2.7.14]
* Supported Windows(R) 8.

[Improvements from Ver 2.7.15]
* Fixed the problem that output process was aborted when a print job had been
  sent from some multithreaded application.

---------------------------------------------------
5. Limitations
---------------------------------------------------
============================
Driver-Specific Limitations
============================

* Local Printer for Microsoft Windows XP, Microsoft Windows Server 2003
  When "\\server\printer\ (LAN Manager port)" is used in the local printer for
  Windows XP and Windows Server 2003, if printing is executed when the printer
  is offline, the local printer may not be able to recover from the offline
  mode.
  If this happens, delete the LAN Manager port and reset the local printer
  settings.
  If LAN Manager port is used in the network printer, there should not be any
  problem.
  When setting the local printer, use other ports except LAN Manager or delete
  the existing LAN Manager port before creating the
  "\\server\printer (local port)" at the "New Port" of the "Add Printer Wizard".

* Installing network printer in Microsoft Windows Vista or later versions
  When installing network printer by [Run as Administrator], the printer may be
  added under the administrator account used for installation and not under the
  current user.

* Driver installation by remote access on Microsoft Windows Vista or later
  versions
  In the case of driver installation by remote access on Windows Vista or later
  versions, the process may not end normally. In such case, try again on 
  Windows XP.

  * Notice to the users in the Microsoft Windows 2000 Server,
    Microsoft Windows Server 2003 and Microsoft Windows Server 2008
    cluster environment
  - Use the following OS for Client.
    Microsoft(R) Windows(R) 2000 (English version)
    Microsoft(R) Windows(R) XP (English version)
    Microsoft(R) Windows Server(R) 2003 (English version)
    Microsoft(R) Windows Server(R) 2008 (English version)
    Microsoft(R) Windows Vista(R) (English version)
    Microsoft(R) Windows(R) 7 (English version)

  - When you specify Custom Paper Size in the cluster environment, make same
    setting at all of the physical node in the environment.

  - When clicking the [Get Information from Printer] button, if the [Search
    Printer] dialog is displayed, select [Specify Address] and enter the
    network address of the printer.

  - Driver Installation in the cluster environment
    (A) Microsoft Windows 2000 Server
        Install the driver on each standby node and active node, and
        then install it on the virtual server.

    (B) Microsoft Windows Server 2003
        Install the driver on the virtual server.

    (C) Microsoft Windows Server 2008
        Install the driver on each standby node and active node from Adding
        Printers, and then install it on the virtual server.
        You cannot use the driver installation tool when installing the driver
        to each node.

  - Driver Deletion in the cluster environment
    (A) Microsoft Windows 2000 Server
        (a-1) Delete the driver on the virtual server.
        (a-2) Delete the driver on each standby node.
        To delete the driver
        Delete the printer icon first and then delete the driver from [Server 
        Properties]. Next, reboot the computer.

    (B) Microsoft Windows Server 2003
        (b-1)  Delete the driver on the virtual server.
        (b-2)  Change standby node to active node.
        (b-3)  Install a printer on the virtual server.
        (b-4)  Delete the driver on the virtual server.
        To delete the driver
        Delete the printer icon first and then delete the driver from [Server
        Properties]. Next, reboot the computer.

    (C) Microsoft Windows Server 2008
        (c-1)  Delete the printer with The Failover Cluster Management.
        (c-2)  Delete the driver with The Failover Cluster Management.
        (c-3)  Delete the printer icon on active node.
        (c-4)  Delete the driver and package from the print server properties
               on active node.
        (c-5)  Change standby node to active node.
        (c-6)  Add a printer with The Failover Cluster Management.
        (c-7)  Delete the printer with The Failover Cluster Management.
        (c-8)  Delete the driver with The Failover Cluster Management.
        (c-9)  Delete the printer icon on active node.
        (c-10) Delete the driver and package from the print server properties
               on active node.

* About the [Cancel] button of [Enter User Details] dialog
  When printing after [Prompt User for Entry when Submitting Job] is set in
  [Detailed User Settings] dialog and the [Enter User Details] dialog is
  cancelled, a warning dialog is displayed.
  It may indicate a printer error message, although there is no error in the
  printer.
  In this case, ignore the warning message and continue operation.

* Number of Copies
  This driver allows you to print from 1 to 9999 copies. Only one copy will be
  printed if the number of copies specified exceeds this range.

* Features of printing with Annotation and Watermark
  When performing watermark printing with [Transparent] specified, some of the
  colors that appear on the screen may be different when actually printed.

  On Windows 8 and later versions, Annotation and Watermark may not be printed
  even if [Annotation] and [Watermark] are specified.
  To make them function, set [EMF Spooling] to [Enabled] on the [Advanced] tab.

* Print Booklet and Print Header/Footer functions
  When the page number printing is simultaneously specified for Print Booklet
  function and Print Header/Footer function, the page numbers may not be
  printed properly.

* Printing Huge Print Data
  For some applications, if a pasted image is printed at high resolution, the
  print data expands and may result in an extremely slow printing speed.
  The print data size of the output may be improved by changing the following
  settings of [Other Settings (Graphics Settings)] on the [Detailed Settings]
  tab.
  - Change [Resolution].
  - Change [Image Compression].

* Black/Color Auto Recognition
  When [Color (Auto)] is specified at [Output Color], though the output may
  appear to be in black, it has been processed in color.
  If you are sure that you want to print in black, specify [Black] at [Output
  Color]. Documents will be printed in color in the following situations.
  - When black and white objects are overlapping the color objects
  - When there are color objects outside the print area
  - When the application uses the system's ICM function to perform color change
  - When the application has its own color change function

* Skip Blank Pages
  Even with [Skip Blank Pages] selected, blank pages may still be printed in
  the following situations.
  - The page contains only line feeds.
  - The page contains only spaces.
  - The page contains only line feeds and spaces.
  - A white background drawing instruction is sent from the application.

* Fax Phonebook File on the Fax tab
  It is recommended to set the [Fax Phonebook File] on the [Fax] tab beforehand,
  using the following way:

  - Open the printing preferences from the printer folder and click [OK] after
    selecting the settings.

  Also, if settings are made on the driver properties screen displayed from the
  application, normally they will be cleared when the application is closed.
  If the settings are made on the [Set / Check Fax Transmission] dialog, they
  will be cleared whenever printing is executed.

* About [Browse and Add Address]
  When a driver (this driver) that supports IP Fax (SIP) data is installed in a
  computer with a fax driver (old driver) that does not support IP Fax (SIP)
  data, part of the display of the old driver will be changed, but operation
  will not be affected.

* Destination numbers of direct fax
  When specifying destination number using wildcards "*" for Speed Dial, the
  maximum number of destinations is not the maximum number of items registered
  on the machine, but it is calculated by the maximum number of items
  displayable using wildcards.

* "Do not display Fax Tab" Checkbox on the "Configuration" tab
  For Windows 2000 ServicePack4 or above, the "Fax" tab may be still displayed
  on the document property of the specific application when "Do not display Fax
  Tab" is checked.
  For Windows 2000 ServicePack4 below, the "Fax" tab may not be displayed on
  the document property dialog under "Printers" folder when "Do not display Fax
  Tab" is checked.

* Blank Separators
  If you set [EMF Spooling] to [Enabled] and perform [2-Sided Print] with documents
  of odd number of pages, a blank page may be inserted on the last page depending
  on application or OS.

* Font Substitution
  If a size equal or larger than 36 points is specified, the document may be
  printed with incorrect font substitution.

* Printing Bold Fonts
  When printing documents with bold fonts, the thickness of characters in the
  Windows 2000 environment may different from the one in other environments.

* Missing Items in the Printout
  In some applications, images may be missing in the printout.
  If this happens, activating EMF spooling as shown below may remove the
  problem.
  - Set [EMF Spooling] to [On] on the [Detailed Settings] tab.

* [Stop Sending] button on the [Set / Check Fax Transmission] dialog
  When you cancel a print job in progress from the driver, the application may
  display a warning dialog.
  It may indicate a printer error message, although there is no error in the
  printer.
  In this case, ignore the warning message and continue operation.

* Specifying Secure Send, F Code and Password
  When [Use Same Cover Sheet for Multiple Recipients] is checked, the Secure
  Send, F code and Password features will be disabled if multiple recipients
  are specified in the [Recipients List].

* Connecting to un-spooled SMB port
  Transmission cannot be done properly when [Use Same Cover Sheet for Multiple
  Recipients] is unchecked and multiple recipients are selected from the
  [Recipients List] if the printer is connected to an un-spooled SMB port.
  This problem may be avoided by setting the SMB port to spool or using other
  ports except SMB port at the printer.

* Custom Paper Size
  Administrator rights are necessary for changing the setting of Custom Paper
  Size.
  When using Windows Vista or Windows Server 2008, please modify printer
  properties according to the following steps.
  - Select the printer from the printer folder.
  - Right-click the printer, click [Run as administrator] and then select
    [Properties].
  - Click the [Continue] button in the [User Account Control] dialog box, and
    from the displayed properties, configure the settings.

  For Windows 7 or later versions select the printer from the [Devices and
  Printers] folder, and select [Properties].
  On the [Sharing] tab, click the [Change Sharing Options] button.
  After that, specify custom page size.

* Favorites
  When only a margin setting is changed, "Change" is not displayed in the
  "Favorites" combo box.

* Printer Error
  An error may occur at the printer if one of the following situations occurs
  during printing. Follow the instructions on the printer UI or the user guide
  to resolve the error.
  - Driver properties from the application program are not displayed.
  - Printer settings on the application program are not reflected in the driver
    properties when displayed.
  - Printer settings are changed midway in a document.
    (E.g. document which has different paper sizes for every page.)
  - Continuous printing from multiple application programs.
  - When an optional device that was not installed to the printer was specified
    at the [Options] tab.

* Compatibility with Printer Font
  If a document using the printer fonts of other machine models is printed
  through this driver, then the results of printing will be different.

* Print Overlay
  The alphabetical [Form Name] specified in the [Print Overlay] is
  case sensitive.
  Specify the correct case sensitive form name registered in the printer.

  As some applications paint the background in white to print, forms with
  overlay may be hidden. Such applications include Internet Explorer and
  WordPad.

* Save to Mailbox
  To use the [Save to Mailbox] feature, a mailbox must be registered in advance
  on the printer. Refer to the machine user guide on how to register mailboxes.
  

* About searching for a printer by [Community Name]
  With the default setting of firewall on Windows Vista or later versions you
  can't search for a printer across subnets by Broadcast.
  In this case, please specify the address directly by selecting Specify Address.

* Image Auto Correction] Feature
  The feature may not function normally depending on applications when documents
  with a large image included are output.

===================
Client Environment
===================

* Multi-language Document
  If a multi-language document is created using the multi-language support
  function, you should select [Always Use TrueType Fonts] on the [Fonts] dialog
  box before printing. When printing with printer fonts, non-Japanese texts
  such as Greek, Croatian, etc. may be printed incorrectly.

=================================
Application-Specific Limitations
=================================

* All Applications
  - Depending on the application used by the customer, blank pages for page
    adjustment will be inserted automatically according to the conditions like
    the number of copies specified when outputting 2-sided prints.
    In this case, the blank inserts will be included by the application.
    The performance is improved by changing the setting below.
    - Check [Skip Blank Pages] on [Advanced Settings] tab. 
  - The print layout may be changed when you change the [Resolution] of this
    driver.
  - In some applications, when the line width is set to thin lines, the
    selected dotted lines may be printed as solid lines instead. If this
    happens, select another line width.
  - When printing documents with image data such as photos, the processing time
    may increase. In such case, the processing time can be reduced by setting
    the [Image Compression] option of [Other Settings (Graphics Settings)] on
    the [Detailed Settings] tab to [Photo].
  - When garbage text is printed, select [Always Use TrueType Fonts] from the
    [Fonts] tab when printing.
  - When text is not printed clearly, it can be improved by changing the
    following setting.
    - Change the [Image Quality] from the [Image Options] tab.
  - When a printed pattern or diagram is different from what you see on the
    screen, changing the following settings of [Other Settings (Graphics
    Settings)] on the [Detailed Settings] tab may alleviate the problem.
    - Uncheck the [High Speed Image Processing].
    - Check the [Gray Guaranteed] check box.
    - Check the [Draw the pattern with fine lines as per the resolution] check
      box.
    - Change [Resolution].
    - Change [Halftone Print].

  You can also improved the problem by changing the following setting:
    - Change the [Print Mode] at the [Graphics] tab.
    - Change the [Image Adjustment Mode] at the [Graphics] tab.
    - Change the [Brightness] and [Contrast], [Chroma] at the [Image Settings]
      tab of the [Graphics Properties] dialog box.

  - The print result may overlap if Multiple Up is selected when printing a
    document that has exceeded the print area of the print/direct fax driver.
  - If the Long Paper document is not printed as shown on the screen, it may be
    improved by setting the [Resolution] to [300dpi] or [200dpi].
  - Setting the following will improve the phenomena if the paper settings from
    the application are incorrect.
    - Modify the [Change Paper Information Handling] setting.

* Output Color Settings from Application
  To print in color from Application of Windows Store, open [Devices and Printers]
  from Windows Desktop, right-click on your printer to select [Printing Preferences]
  and then confirm that [Output Color] on the [Basic] tab of the [Printing Preferences]
  dialog is set to [Color].
  If the setting of [Output Color] on the [Basic] tab of the [Printing Preferences]
  dialog remains [Black and White], the output will be in black and white even
  if you specify Color Mode to [Color] on the printing setting screen shown
  after you select printer from the device charm.

* Adobe Acrobat
* Adobe Reader
  Changing the following settings may improve the printing result if the
  printed output is different from what you see on the screen.
  - Check the [Print Image] at the print dialog box of the application before
    printing.

  When printing a PDF file containing mixed sizes such as A4 portrait and A3
  landscape, the print/direct fax driver is unable to separate and print pages of
  different sizes onto different paper in a single operation.
  To print on different paper sizes, separate the pages of different sizes into
  different print operations.
  To fit a mixed-size print output to a single paper size in a single print
  operation, select [Reduce] on the [Print] dialog box.
  For example, you can rotate and reduce an A3 landscape page to be printed on
  an A4 portrait paper.

  [Image Rotation 180 Degrees] setting will not be reflected on the output
  result.

* Adobe Illustrator 9.0
  [Paint] and [Lines] areas specified in the text may be printed incorrectly if
  printer fonts are used.
  If this happens, specify [Always Use TrueType Fonts] on the [Fonts] tab in
  the print/direct fax driver.

* Adobe Illustrator 10.0.3
  When a printed pattern or diagram is different from what you see on the
  screen, the problem may be improved by changing the settings of [Other
  Settings (Graphics Settings)] on the [Detailed Settings] tab.
  - Set [Resolution] to [600dpi].
  - Set [Halftone Print] to [On].

* Adobe Illustrator 12.0
  When [High Resolution] is selected for [Print Mode], unwanted lines may be
  printed. The print result may be improved by selecting [On] for [Print as
  Bitmap] in the print dialog of an application.

* Adobe PageMaker
  Images pasted at a tilted angle may be printed with dotted line grids.

* CorelDRAW
  If a printed pattern or diagram is different from what you see on the screen,
  you can improve the result by the following settings.
  - Change [Print Mode] in the [Graphics] tab.
  - Change the following settings in [Other Settings (Graphics Settings)] in
    the [Detailed Settings] tab.
    - Set [Halftone Print] to [On].
    - Set [Paint Only Enclosed Areas] to [On].

* Corel Designer
  Objects that are drawn in solid lines may be printed in dotted lines.
  The print output may not look good, for example, lines and gaps may be seen
  in circle gradations.
  The print output may be improved by converting the gradations to images.

* JustSystems Ichitaro
  Sometimes the partial printing may not be performed properly. Such cases can
  be avoided by the following method.
  - Before starting the application, open the default setting of the document
    from the Printer Folder and click [OK].

* Microsoft Excel
  When printing a book or multiple sheets in Excel, the second and subsequent
  sheets may not be printed as specified in the dialog settings.
  When you specify to print an entire book with mixed double-sided and
  single-sided sheets, each sheet is printed according to its individual print
  information. Batch printing is not performed. You can avoid this problem by
  doing the following:
  1. Select another printer on the print dialog or page setup dialog of any
     sheet and close the document temporarily to activate the change.
  2. Change the default value of the driver to the desired setting.
     (E.g. 2 Sided Print, 2 Up, etc.)
  3. Open the document and select this driver on the print dialog before
     printing.

  The print layout may be changed when you change the [Resolution] of this
  driver.

  When sending a fax document as a book or in multiple sheets in Excel, the
  document may be faxed as per sheet as instructed by Excel.
  In this case, select [Start Sending] after checking each setting on the
  [Set/Check Fax Transmission] dialog which will be displayed more than once.
  Please note that jobs with the [Stop Sending] button selected will not be
  faxed.

  You may not be able to print if you change the port after installing this
  driver. In this case, delete the driver.Specify the desired port and install
  again.

* Microsoft Internet Explorer
  When the output of the image data is different from what you see on the
  screen, use the following method to resolve.
  - Change the [Resolution] setting of [Other Settings (Graphics Settings)] on
    the [Detailed Settings] tab.

  If a Web page containing Excel document is printed in multiple parts, you can
  rectify the problem using the following methods.
  1. Quit Internet Explorer.
  2. Open printer properties in the Printers folder.
  3. Switch [Apply Zoom to Application] to [Off] in the items list of [Other
     Settings (Graphics Settings)] in the [Detailed Settings] tab.

  Since File creation at printing is restricted on Internet Explorer in
  Protection mode on Windows Vista or later versions Form file can not be
  created even if [Create/Register Forms] is specified.

  When sending Direct FAX from Internet Explorer in Protection mode on Windows
  Vista or later versions after clicking the [Phonebook Tool] button in the 
  [Set/Check Fax Transmission] dialog, a warning message of Internet Explorer
  Security may be displayed. Click "Allow" and continue.

  When outputting from Internet Explorer in Protection mode on Windows Vista
  or later versions the pop-up detailed user settings and a part of changes
  made in the [Set/Check Fax Transmission] dialog are not taken over to the
  output next time.

  The following functions are restricted with use of Internet Explorer in
  Protected Mode on Windows Vista or later versions.

  - The setting items for [Job Type] ([Secure Print] / [Sample Set] / [Delayed
    Print] / [Store in Remote Folder]) can not be edited.
  - The functions of [Saved Settings], [Save] and [Edit] are disabled.
  - The functions of [Watermark], [New], [Edit] and [Delete] are disabled.
  - The setting of [Notify Job Completion by E-mail] can not be changed.
  To change the settings of these functions, open the default setting of the
  document from the Printer Folder.

* Microsoft PowerPoint
  Depending on the font (e.g. MS-Mincho) and point size specified for a piece
  of text, the underscore (_) and the underline may overlap in the print output.
  Even if the overlap is not apparent because of the screen display ratio, the
  underscore (_) and the underline may overlap on the print output.

  When the output in black is different from what you see on the screen, use
  the following method to resolve.
  - Check the [Grayscale] on the Print dialog of the application and print.

* Microsoft Visio
  Setting the following will improve the problem of printing subsets of various
  sizes in which is different from the specified [Paper Size] in [Basic] tab.
  - Set [Change Paper Information Handling] to [On] on the [Detailed Settings]
    tab.

* Microsoft Word
  Even if [Skip Blank Pages] is specified, when a blank page is included in
  documents, it may be output.

  When [Poster] is selected to print two or more copies of a single-page
  document, the copies will not be collated.

  You may not be able to print if you change the port after installing
  this driver. In this case, delete the driver.
  Specify the desired port and install again.

* Lotus Freelance
  Some of the settings such as paper source, print mode in the printer
  properties may not be reflected in the output.

* PCA Account EX-V
  The recipient cannot be set if the direct fax driver is selected from the
  Printer Settings dialog box.

* Fuji Xerox DocuWorks
  When printing a mixed size document, the printer may not be able to switch
  between different output paper sizes. Such cases can be avoided by the
  following method.
  - Display the [Printer Settings] dialog box using the [File] >
    [Printer Settings] menu.
  - Specify [Auto] from [Paper Source].

  If the direct fax driver is used as an easy printer, the recipient specified
  at the properties will be disabled.
  Specify the recipient on the [Set / Check Fax Transmission].

  In Ver 5.x or earlier, please note that if easy printer of a FAX model is
  created from Properties on the [Printer Settings] screen, the address last
  specified may be retained when sending a fax.

---------------------------------------------------
6. Inquiries
---------------------------------------------------
Fuji Xerox Co., Ltd.
Customer Contact Center

Please check the telephone number to call on the
"Maintenance/Operation Inquiries" card pasted on the machine.

    The latest software is available on our web site.

        http://www.fujixerox.co.jp/download/

    Communication charges will be borne by the customer.

-------------------------------------------------------------------------------
Microsoft, Windows, Windows Server, Windows Vista, Word, Excel, PowerPoint,
Internet Explorer and Visio are either registered trademarks or trademarks
of Microsoft Corporation in the United States and/or other countries.

Adobe, Acrobat, Illustrator, PageMaker and Reader are
either registered trademarks or trademarks of
Adobe Systems Incorporated in the United States and/or other countries.

XenApp is a trademark or a registered trademark of Citrix Systems, Inc.
in the United States and other countries.

CentreWare is a registered trademark of Xerox Corporation.
DocuWorks is a registered trademark of Fuji Xerox Co., Ltd.

Other company names and product names are trademarks or registered
trademarks of the respective companies.

This software is based in part on the work of the Independent JPEG Group.

(C) Fuji Xerox Co., Ltd. 2008-2015
