
       ----------------------------------------------------
       
            Files for IBM Infoprint  1226 PCL Drivers
       
               for use with Microsoft Windows XP
       
       ----------------------------------------------------


    1. Version History:   Initial Release


    2. Contents:
       Filename           Description
       ------------       -----------
       readme.1st         This file
       iiaada40.inf       Setup file for installation
       iiaada40.dll       Unidriver Resource DLL File
       iiaada40.gpd       Unidriver GPD File
       iiaada40.cat       Security Catalog File


    3.  Installation Instructions:

       Step 1: Preparation

          1. Format a diskette or create a folder on the hard disk and copy
             the files in this package to it.  This diskette or location will
             be referred to as the IBM Driver Disk for the remainder of
             these installation instructions.

       Step 2: Update / Installation

             To install or update one of the printers listed above, take the
             following steps:

             1. Select the "Start" button on the task bar. Then select "Printers 
		and Faxes". Then select "Add a printer". Select "Next>".

             2. Select "Local printer attached to this computer". Uncheck 
		"Automatically detect and install my Plug and Play printer". 
		Select "Next>".

             3. Select the port to be used by this printer. Select "Next>".

             4. The default list of printers supported by WinXP will now appear. 
		Select "Have Disk..." button. Select "Browse..." button and locate 
		the package.

             5. Select iiaada40.inf from the list of available INF files.  Choose
                "Open".  Then, choose "OK".

             6. Select your printer from the list that appears and select
                "Next>".

             7. If this printer is already installed on your system, you must
                choose to either keep the existing driver or replace with the
                new driver.  A second print object with a different name will
                be added for the new printer.  Choose "Next>".

             8. Enter the name you wish to appear for your printer or leave the
                default if you wish.  Decide if this printer will be the
                default printer.  Select "Next>".

             9. If you do not wish to share your printer on a network, leave the 
		"Do Not share this printer" button marked and choose "Next>". 
		Otherwise, select the "Share as" radio button and enter the name 
		you wish to assign to this shared printer.  Then choose "Next>".
		Then, if you wish, enter the location of this printer and/or any
            	comments to associate with the printer and choose "Next>".
		                
            10. You now have the option to print a test page in order to test
                the configuration of your printer.  After making this decision,
                choose "Next>".
                
            11. Choose "Finish" to begin copying files for the installation.If 
                prompted for files during the installation process, point
                to the drive or folder containing your IBM Driver Disk.
      
            12. You can now setup your printer by going to the Printers folder
                and right-clicking on your printer's icon.  From the menu that
                appears, choose Properties.  When you have made all of the
                desired changes choose "OK" to save your settings.




