README.TXT
===========================================================================
 
                         Microsoft Windows
                        Color Correct Utility

                          Version 1.0.0

              Copyright(C) 2003  Oki Data Corporation
===========================================================================

 TABLE OF CONTENTS
 1. Features
 2. Operating environment
 3. How to use at printing
 4. Notes
 5. How to delete
 6. Release History
 *Trademarks


 ===========================================
 1. Features
 ===========================================
 Color Correct Utility provides color Correct methods for the following
 purposes.

 - To match the print result colors to the palette colors (specific colors on
   the screen).
 - To adjust Gamma, Hue, Lightness, and Saturation.

 Note)
 In order to print in the colors registered by the utility, you have to select
 the setting name when you print. For details, refer to "3. How to use at
 printing."


 ===============================================
 2. Operating environment
 ===============================================
 PC on which Windows Me/98/95, Windows NT4.0, Windows 2000 or Windows XP
 operates

 Compatible printers
 - Jolimark LP- C2024,C3037,C3037Pro series,
 - Jolimark LP- C1220
 For details about how to use, refer to the manual or Help of the utility.


 =================================
 3. How to use at printing
 =================================
   Jolimark LP- C2024,C3037,C3037Pro series, Jolimark  LP-C1220
 
 - PostScript Driver
 (1) Start the application.
 (2) Select [Print] in [File] menu.
 (3) Click [Properties]. 
 (4) Check [User Setting] in [Color Setting] in [Color] Tab. 
     Select the Color Correct Name you registered in the Color Correct
     Utility.)
 Note: This is valid only when you set [Color Control] to [OKI Color
       Matching].

  - PCL Driver, Jolimark  LP-C1220 Driver
 (1) Start the application.
 (2) Select [Print] in [File] menu.
 (3) Click [Properties]. 
 (4) Select [Manual Color] in [Color Mode] in [Color] Tab.
 (5) Check [Use Setting] in [Color Setting]. Select the Color Correct Name 
     you registered in the Color Correct Utility.


 =================================
 4. Notes
 =================================
 (1) You need to register Color Correct for each printer driver.

 (2) Color Correct is not applied to print data based on CMYK color space.

 (3) When you click [Print Color Sample] or [Print Current Colors], the sample
     is printed on the paper placed in the tray selected in [PRINT MENU]-
     [PAPER FEED] in printer operation panel (default: Tray 1). The data of
     the sample print is made so that it fits B5 or bigger size paper. 
     Set B5 or bigger paper in the selected tray.

 (4) The Color Correct Utility is not used for the Shared Printer.


 ========================================
 5. How to delete
 ========================================
 (1) Select [Control Panel]-[Add/Remove Programs].
 (2) Select [Jolimark Color Correct Utility] and delete it.


 =================================
 6. Release History
 =================================
 - Ver 1.0.0 (07/03/03) First Release
 
 =================================
 *Trademarks
 =================================
 Company names and product names in this document are registered trademarks
 or trademarks of the various companies. 


 End.

