15.Product Specifications

|  | Note: | • Specification values vary slightly from printers with different models with different functions ,and product specifications vary from different countries and regions. • These values are based on the initial data. For more information about the latest specifications, please visit: www.pantum.com.

15.1.Overview of the Specifications

Product Size(W*D*H) | 415mm*360mm*352mm
Printer weight (excluding powder box, drum module and package) | About 10.54kg
Weight of printer (including cartridge, drum and package) | About 13.71kg
Touch screen | Dimension: 3.5" capacitive touch screen
Resolution: 320*480, RGB565
Print Environment | Print temperature range:10-32℃
Print humidity range:20%RH~80%RH
Power Voltage | 110V Model: AC100~127V, 50Hz/60Hz,9A
220V Model: AC220~240V, 50Hz/60Hz,4.5A
Noise (acoustic pressure level) | Print/scan: ≤52dB(A)
Copy: ≤54dB(A)
Standby: ≤30dB(A)
Mute mode: ≤46 dB (A)
Enter network standby time: | 5 minutes
Power Consumption
Standby: ≤ 50W
Shutdown: ≤ 0.5W
Network standby: The model with wireless function: 2.366W The model without wireless function: 1.888W
Operating System | Microsoft Windows XP/ Windows Vista/ Windows 7/ Windows 8/ Windows 8.1/ Windows 10/ Windows Server 2003/ Windows Server 2008/ Windows Server 2012（32/64 Bit）
macOS 10.8/10.9/10.10/10.11/10.12/10.13/10.14/10.15
Linux ：Ubuntu 14.04/16.04/18.04（32/64 Bit）
iOS 9.0-12.0
Android 4.4-9.0
Communication interface | Hi-speed USB 2.0
IEEE802.3 10Base-T/100Base-Tx
IEEE802.11b/g/n (support WPS)

15.2.Print Specifications

Print Speed | 33ppm(A4)/35ppm(Letter)
Print Time of First Page | ≤8.5sec
Print Language | PDL

15.3.Copy Specifications

Copy Speed | 33cpm(A4)/35cpm(Letter)
FCOT | Flatbed <10 seconds ADF <12 seconds
Maximum Pages for Successive Print | 99 pages
Zoom Ratio | 25%~400%
Other Copy Functions | ID copy, bill copy, multi-in-one copy, clone copy.

15.4.Scan Specifications

Scan Type | Flatbed+ADF
Scanning speed | Single-sided: 24ipm Duplex: 48ipm
Maximum Scan Size | Flatbed: 216×297mm ADF: 216×356 mm
Chromoscan | Yes
Scan Output Function | Scan to E-mail, PC, FTP and USB

15.5.Fax specification

Fax Type | Black-and-white
Modem Speed | 33.6Kbps
Fax Memory | 650 pages
Encoding | MH/MR/MMR/JBIG
Compatibility | ITU-T sg3/ECM
Resolution | Standard, fine, super fine, picture
Other Fax Functions | PC-FAX (Send), Fax Filtering, Group Sending, Fax Forwarding, Speed Dial, Group Dial, Delay Sending, Auto Redial, Auto Receive, Auto Shrink, Mobile Fax
Environment | PSTN、PABX、VOIP

Company Name: Magnell Associate, Inc. ( DBA NEWEGG.COM ) Office address:17560 Rowland St. City of Industry, CA 91748 TEL: （626）271-9700 USA Only