7.Print

7.1.Print Function

You can set the print function through "Start"-"Devices and Printers"- select corresponding printer- right click – set print function in "Printing preferences". Some functions are as follows:

Functions | Diagram
Automatic Two-Sided Printing |
Collate Print |
Reverse Print |
N-in-1 |
Poster Print(for Windows Operation System only) |
Zoom Print |
Custom Size |

| Note： | • Windows 7 is taken as example in the above description. • You can realize poster printing feature by selecting 2x2 poster printing in multipage. • You can enable printing preference and click the help button to view detailed function description. Please refer to Chapter 7.9 for the method to open help document.

7.2.Print Settings

You can set up printing parameters with the following two methods before sending printing work (such as paper type, paper size and paper source).

Operating system | Temporary printing setup change | Permanent default setup change
Windows 7 | 1. Click “File” menu – “Print” – “Select printer" - “Printer properties” (the detailed steps may differ because of multiple operating systems). | 1. Click “Start” menu- “Control Panel” – “Devices and Printers”. 2. Right click on the printer icon, select “Printing preference” and then change setup and save it.
Mac OS | 1. Click “File” menu – “Print”. 2. Change setup in the window popping out. | 1. Click “File” menu – “Print”. 2. Change setup in the window popping out and click to save the preset. (Select preset every time before printing, or print according to default setup.)

| Note： | • Priority of App setup is senior to printer setup.

7.3.Cancel printing

The current printing work can be cancelled in printing process. As for printers with LCD control panel, the current printing work can be cancelled by pressing “Cancel”; as for printers with LED control panel, the current printing work can be cancelled by pressing the “Cancel” key for more than 2s.

7.4.Printing Mode

The printer can print with auto feed tray and manual feed tray. The defaulted state is auto selection, and if there is printing medium in the manual feed box, papers in manual feed tray will be used with priority.

7.4.1.Printing with the Automatic Feeder Tray

Before printing, please make sure mediums of corresponding quantity have been installed inside the auto feed tray, and there is no printing medium in the manual feed tray.

| Note： | • For precautions on loading paper, see Chapter 2. • For the type of media to be printed with the automatic feeder tray, see Chapter2.1.

7.4.2.Printing with manual feed tray

When you put papers in the manual feed tray, the printer will enter manual feed mode.

| Note： | • Manual feed mode means that papers will be fed from the manual feed tray first if there are papers being put inside it. • Generally, the manual feeder tray is used to print on special paper, such as envelopes, transparencies, etc., and only one piece of paper can be loaded each time. • Please refer to Chapter 2 for putting papers inside manual feed tray. • Please refer to Chapter 2.1 for type of mediums that can be printed via manual feed tray.

7.5.Automatic Two-Sided Printing

The printer supports automatic two-sided printing of plain paper. Paper size supported by the automatic two-sided printing: A4,Letter, Legal, Oficio, Folio,16K.

| Note： | • Trying the automatic two-sided printing may damage the printer if some paper media are not suitable for automatic two-sided printing. • Auto duplex printing does not support poster printing. • Please refer to Chapter 2 for paper loading and type of mediums that can be printed via auto feed tray.

7.5.1.Duplex printing unit setup

For the purpose of achieving the best printing result, you can set up the paper size of duplex printing unit. As for duplex printing of A4 and 16K papers, the slide should be adjusted to the A4 position; as for Letter, Legal, Folio and Oficio duplex printing, the slide should be adjusted to the Letter position.

Setup steps of duplex unit are:

1. Draw out duplex unit.

2. Make the backside of duplex unit up.

3. Adjust paper size slide to A4 or Letter position to finish setting up.

4. Install the duplex unit in the printer.

7.5.2.How to carry out auto duplex printing

1.Open the print job to be printed from the application (such as a Notepad).

2.Select Print from the File menu.

3. Select printer of the corresponding model.

4. Single click “Preferences” for printing setup.

5. Select the “Duplex” in “Basic” tab and then select “Long Edge” or “Short Edge”.

6. Single click “OK” to finish printing setup. Click “Print” to realize auto duplex printing.

7.6.Fine mode printing

The Fine mode is applicable to engineering drawings and fine lines printing.

Set up fine mode in the basic page of printer preference After setup, fine printing mode can be realized.

7.7.Mute printing

If the Mute Printing is set, the printing noise will be reduced but the printing will slow down to some extent.

The operating steps of mute printing are as follows (applicable to printers that are installed via USB connection)

Windows 7 is taken as the example in the following operation. The information on your computer screen may differ because of multiple operating systems.

1. Enter the “Start menu” – “Control Panel” –view “Devices and Printers”.

2. Right click printer and select “Printer properties” in the pull-down menu.

3. Enter the “Secondary Settings” option.

4. Tick “Mute printing” and click “Ok” to finish setup.

5. Open the printing work from the App, select a printer of the corresponding model and then set up printing according to needs.

6. Click “Print” to realize mute printing.

| Note： | • Printers with LCD control panel can be set to mute printing with keys on control panel directly, please refer to Chapter 9.1.4.

7.8.Auto shut-off setting

“Auto shut-off setting” to set off condition and off delay of printer.

1. Enter computer “Start Menu” – “Control Panel” – View “Devices and Printers”.

2. Right click printer, select “Printer properties” in drop-down list.

3. Enter “Secondary Settings” option and set “Auto shu-off setting”.

4. Click “OK” to finish setting.

| Note: | • For printer provided with LCD control panel, users may set auto off function through control panel keys. Please refer to Chapter 9.1.6. • Individual countries (or regions) do not support auto off setting.

7.9.Open Help Document

You can open the "Printing preferences" and click "Help" button (for Windows Operation System only). The help document contains the user guide where you can find the information on print settings.