************************************************************************
SOFTWARE LICENSE AGREEMENT
THIS AGREEMENT (or "EULA") IS A LEGAL AGREEMENT BETWEEN THE PERSON, COMPANY, OR ORGANIZATION THAT HAS LICENSED THIS SOFTWARE ("YOU") AND RICOH CO. LTD. BY INSTALLING AND/OR USING THE SOFTWARE, YOU AGREE TO BE BOUND TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO BE BOUND BY THESE TERMS, THEN DO NOT INSTALL AND/OR USE THE SOFTWARE. 
License Grants
This software is only licensed for use with the equipment it was packaged with. This software cannot be rented or leased to a third party.
License Duration
This license is effective for as long as the software remains on your computer or until terminated. License termination will be considered implicit if the terms of the license agreement are breached. Upon termination of the license agreement, this software must be removed from your system and all copies of this software and its documentation must be destroyed.
Ownership of this Software
You own, at most, only the media on which the software resides.
Copying
This software and its documentation are the subject of copyright. You may not make any copies of the software except as necessary for licensed use. Any such copies are subject to the conditions of this Agreement.
You may not modify, adapt, translate, reverse engineer, decompile, disassemble or create any works based in whole or in part on this software or its documentation.
You may be held legally responsible for any copyright infringement, unauthorized transfer, reproduction or use of the software or its documentation.
Warranty
The software is provided as is with no implicit guaranty of quality or fitness for any particular use. If the software was distributed on physical media such as a CD-ROM, any defects in the physical media are covered under warranty for a period of 1 year. IN NO EVENT SHALL THE SUPPLIER OF THIS SOFTWARE OR ITS LICENSORS BE HELD LIABLE FOR DAMAGES. THIS INCLUDES ANY DAMAGES RESULTING DIRECTLY OR INDIRECTLY IN THE LOSS OF INFORMATION, PROFITS, SAVINGS, OR INTERRUPTION OF BUSINESS FROM THE USE OR INABILITY TO USE THIS SOFTWARE.
Exportation
Exportation of this software is governed by the export control laws of the United States and other countries. You agree to comply with all such export control laws.
Legal Provisions
If any part of this Agreement is found to be illegal, invalid or unenforceable, the remaining provisions shall remain in full effect.
************************************************************************

--------------------------------------------------------------------
                 Microsoft Windows XP SP2 or later
      Windows Server 2003/Windows Server 2003 R2/Windows Vista
        Windows Server 2008/Windows 7/Windows Server 2008 R2
                 SAVIN PCL minidriver Version 2.17
                               2012/11
--------------------------------------------------------------------
This driver can also be used for 64-bit editions of Windows.

--------------------------------------------------------------------
    SUPPORTED MODELS
--------------------------------------------------------------------
  2015DP, 2055DP, 2070DP, 2085DP, 2105DP, 2512, 2513, 2513f, 2515,
  2518, 2518d, 2522, 2527, 2532, 2535/2235, 2545/2245, 2555, 2560, 
  2575, 2585, 25105, 4035/4135g, 4045/4145g, 4090, 40105, 
  4022, 4027, 4035e/4135eG, 4045e/4145eG, 4051, 4060, 
  4075,
  9918DP, 9922DP, 9927DP, 9935D, 9935DP/2035DP, 9935DPE/2035DPE,
  9945DP/2045DP, 9945DPE/2045DPE, 9955DP, 9965DP, 
  SLP14, SLP16, SLP20, SLP21, SLP26, SLP26n, SLP27, SLP32, SLP45,
  MLP45, MLP26, MLP26n, MLP32, MLP25, MLP25n,
  FAX 3725, 3725e, 3730, 3799/3799nf, 3750, 3760, 3770,
  3750nf, 3760nf, 3770nf,
  C2408, C3210, CLP1036, CLP1620, CLP28, SLP38c,
  C2524, C2532,
  4015, 4018, 4018d, 3515,
  MLP28, MLP28n, MLP35n, MLP75n,
  C3224, C3828, C2820,
  CLP17, CLP18, CLP35, CLP831,
  CLP26DN, CLP128, CLP135,
  C2824, C3528, C4535, C6045, SDC555, C2410, C3210e,
  8025, 8030, 8035/8035g, 8045/8045g,
  8016, 8020, 8020d, CLP22,
  8090, 8110, 8135, 8055, 8065, 8075, MLP145,
  C2525, C3030, SGC 1506, CLP27DN, CLP31DN,
  C3535, C4540, CLP240D,
  MLP175n, 9016, 9021d, 8025e, 8030e,
  8035e, 8045e, 816, MLP31n, MLP36n, 7025,
  SP C400DN, C2020,
  C6055, C7570,
  9025, 9025b, 9033, 9033b, 
  9040, 9040b, 9050, 9050b,
  SP C420DN,
  8060, 8070, 8080,
  MLP150DN,
  MLP31nL,
  CLP131DN,
  Pro 906EX, Pro 1106EX, Pro 1356EX,
  C9020, C9025,
  C2828, C3333,
  C4040, C5050,
  CLP340D, CLP350D,
  C9020L,
  MLP37N,
  917,
  Pro 907EX, Pro 1107EX, Pro 1357EX,
  9060, 9070, 9080, 9090,
  MLP235n,
  C9065, C9075,
  9240, 9250,
  9228, 9233,
  CLP37DN, CLP42DN,
  C9145, C9155, C9145A, C9155A,
  C9130, C9135,
  C9120, C9125,
  920,
  C 230, C 230SR, C 240, C 240SR,
  SP C320DN,
  SP 4310N,
  SP 5200DN, SP 5210DN,
  SP 5200S, SP 5210SF, SP 5210SR,
  MP 2352, MP 2852, MP 3352,
  MP C4502, MP C5502, MP C4502A, MP C5502A,
  MP C3002, MP C3502,
  MP 301,
  MP 4002, MP 5002,
  MP C305,
  MP 6002, MP 7502, MP 9002,
  SP C830DN(NEW), SP C831DN(NEW),
  SP 8300DN(NEW)

--------------------------------------------------------------------
    NOTE
--------------------------------------------------------------------
Introduction
This readme explains the installation and removal procedures for this PCL-mini driver. The end of this readme contains some important notes about the use of this driver. Please read this carefully before installing the PCL-mini driver.

Contents
1 Installing the PCL-mini driver
2 Uninstalling the PCL-mini driver
3 Upgrading the PCL-mini driver to a newer version
4 Notes
========================================================================

1 Installing the PCL-mini driver
As the information contained in this document applies to multiple print devices, the word "Device" is used as a generic reference to whichever device you are using.
	1-1 For devices connected via USB
		1-1-1 Windows 7, Server 2008 R2
		Step 1 Log in to Windows as an Administrator.
		Step 2 Close any open applications.
		Step 3 Connect the "Device" to a PC using a USB cable and then power on the "Device".
		Step 4 Automatic installation of the device driver will appear to start and then fail, displaying the message "Device driver software was not successfully installed". Close this message.
		Step 5 Open "Device Manager".
		Step 6 The "Device" should be listed under "Other devices". Right-click "Device" and select "Update Device Software...".
		Step 7 When the "Update Device Software" screen is displayed, select "Browse my computer for driver software".
		Step 8 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
		Step 9 Follow the rest of the Wizard's instructions to complete the installation. A warning "Digital Signature Not Found" might be displayed during installation. If so, please just ignore this message and continue with the installation.
		
		1-1-2 Windows XP, Vista, Server 2003, 2003 R2, 2008
		Step 1 Log in to Windows as an Administrator.
		Step 2 Close any open applications.
		Step 3 Connect the PC and the "Device" using a USB cable and then power on the "Device".
		Step 4 If a "Found New Hardware" popup is displayed, click "Cancel" to close it.
		Step 5 Open "Printers and Faxes" from the Start menu.
		Step 6 Select "Add Printer".
		Step 7 "Welcome to the Add Printer Wizard" is displayed. Click "Next >".
		Step 8 The "Local or Network Printer" dialogue is displayed. Select "Local printer attached to this computer" and click "Next >". Note: Do not enable "Automatically detect and install my Plug and Play printer".
		Step 9 The "Select a Printer Port" dialogue is displayed. Select "Virtual printer port for USB" as the port type.
		Step 10 The "Install Printer Software" dialogue is displayed. Select "Have Disk".
		Step 11 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
		Step 12 Follow the rest of the Wizard's instructions to complete the installation. A warning "Digital Signature Not Found" might be displayed during installation. If so, please just ignore this message and continue with the installation.
       
	1-2 For devices connected via network
		1-2-1 Windows 7, Server 2008 R2
		Step 1 Log in to Windows as an Administrator.
		Step 2 Close any open applications.
		Step 3 From the "Start" menu, select "Devices and Printers" > "Add a Printer".
		Step 4 The "Add a Printer" dialogue will be displayed asking "What type of printer do you want to install?" Select "Add network, wireless, or Bluetooth printer".
		Step 5 The "Searching for available printers" dialogue appears. Select the "Device" from the list of printers and click "Next". (If you do not see your "Device" in this list, please proceed to "What to do if your device is not found" at the end of this section.)
		Step 6 The "Install the printer driver" dialogue appears. Click "Have Disk".
		Step 7 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
		Step 8 Follow the rest of the Wizard's instructions to complete the installation. A warning "Digital Signature Not Found" might be displayed during installation. If so, please just ignore this message and continue with the installation.
		
		1-2-1-b What to do if your device is not found
		Step 1 Log in to Windows as an Administrator.
		Step 2 Close any open applications.
		Step 3 From the "Start" menu, select "Devices and Printers" > "Add a Printer".
		Step 4 The "Add a Printer" dialogue will be displayed asking "What type of printer do you want to install?" Select "Add a local printer".
		Step 5 The "Choose a printer port" dialogue will be displayed. Create a new "Standard TCP/IP Port" and click "Next".
		Step 6 Enter the "Device" IP address and uncheck "Query the printer and automatically select the driver to use". Click "Next".
		Step 7 The "Install the printer driver" dialogue appears. Click "Have Disk".
		Step 8 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
		Step 9 Follow the rest of the Wizard's instructions to complete the installation. A warning "Digital Signature Not Found" might be displayed during installation. If so, please just ignore this message and continue with the installation.

		1-2-2 Windows XP, Vista, Server 2003, 2003 R2, 2008
		Step 1 Log in to Windows as an Administrator.
		Step 2 Close any open applications.
		Step 3 Open "Printers and Faxes from the Start menu.
		Step 4 Select "Add Printer".
		Step 5 "Welcome to the Add Printer Wizard" is displayed. Click "Next >".
		Step 6 The "Local or Network Printer" dialogue is displayed. Select "Local printer attached to this computer" and click "Next >". Note: Do not enable "Automatically detect and install my Plug and Play printer".
		Step 7 The "Select a Printer Port" dialogue is displayed. Select "Create a new port" > "Standard TCP/IP Port" as the port type and click "Next >".
		Step 8 The "Add Standard TCP/IP Printer Port Wizard" is displayed. Click "Next >".
		Step 9 Enter the device IP address or hostname and click "Next >".
		Step 10 The "Install Printer Software" dialogue is displayed. Select "Have Disk".
		Step 11 Browse to the folder containing the driver files (typically the CD-ROM or an extracted archive downloaded from the website) and click "OK".
		Step 12 Follow the rest of the Wizard's instructions to complete the installation. A warning "Digital Signature Not Found" might be displayed during installation. If so, please just ignore this message and continue with the installation.
	
2 Uninstalling the PCL mini-driver
	2-1 Windows 7, Server 2008 R2
	Step 1 Log in to Windows as an Administrator.
	Step 2 Close any open applications.
	Step 3 Open the "Devices and Printers" folder from the "Start" menu.
	Step 4 Delete the printer icon corresponding to the driver that is to be uninstalled.  
	Step 5 File > Server Properties > Driver tab.
	Step 6 Click the "Change Driver Settings" button.
	Step 7 Select the driver to be uninstalled.  
	Step 8 Press the Delete key.  
	Step 9 Log the current user account off.

	2-2 Windows Vista, Windows Server 2008
	Step 1 Log in to Windows as an Administrator.
	Step 2 Close any open applications.
	Step 3 Click the "Printer" icon in the "Control Panel".
	Step 4 Right-click anything in the folder and select "Run as administrator".
	Step 5 Delete the printer icon corresponding to the driver that is to be uninstalled.  
	Step 6 File > Server Properties > Driver tab.
	Step 7 Select the driver to be uninstalled.  
	Step 8 Press the Delete key.  
	Step 9 Log the current user account off.

	2-3 Windows XP, Windows Server 2003, 2003 R2
	Step 1 Log in to Windows as an Administrator.
	Step 2 Close any open applications.
	Step 3 Click the "Printer" icon in the "Control Panel".
	Step 4 Delete the printer icon corresponding to the driver that is to be uninstalled.  
	Step 5 File > Server Properties > Driver tab.
	Step 6 Select the driver to be uninstalled.  
	Step 7 Press the Delete key.  
	Step 8 Log the current user account off.


3 Upgrading the PCL mini-driver to a newer version
	Step 1 Delete the existing driver using the procedure described in "2 Uninstalling PCL printer driver".
	Step 2 Install the new version of the driver using the procedure described in "1 Installation of the PCL printer driver".
	Step 3 Restart.

4 Notes
	- In order to use the "Update Now" function for Automatic Configuration, the SNMP community name must be "public".
	- Some devices do not support the use of settings such as duplex, staple, punch and z-fold with custom paper sizes.
	- Booklet settings and Page per Sheet Layout settings have no effect in Windows XP SP3. As a result, the default settings (*) are always used.
		- Booklet Binding Edge
			- On Left Edge (*)
			- On Right Edge
		- Pages per Sheet Layout
			- Right then Down (*)
			- Down then Right
			- Left then Down
			- Down then Left

	- An extra page is added to the end of odd-paged duplex jobs. The added page might be incremented in the printer's counter.
	- Black and White documents might be printed in full color (CMYK). To ensure that the job prints using pure Black (K), please change the color mode to "Black and White" or "Monochrome".
	- Watermarks are not supported on some operating systems.
	- The Draw Border function is always on if usings Windows XP SP2 or earlier.
	- In order to use the "Update Now" button for Automatic Configuration, a Standard TCP/IP port must be used and all 3 of the following conditions must be met:
		- Protocol: Raw
		- SNMP Status Enabled checkbox: on
		- SNMP "Community Name": public

========================================================================

All brand names and product names mentioned in this document are trademarks or registered trademarks of their respective companies.

