Language:
Welcome to TESORO World
Congratulations on purchasing your very own TESORO GUNGNIR™ Optical Gaming Mouse - a gaming mouse engineered to suit the needs of
every gamer. Featuring powerful macro editor function enable users to record the mouse and keyboard actions. It is the mouse of choice for
optimizing the gaming experience.
3500 DPI Gaming Optical Sensor with high speed motion detection and acceleration
7 independent programmable buttons
Adjustable 4 levels DPI control: 450/900/1800(Default)/3500
Adjustable polling rate control from user AP up to 1000Hz ultra-polling rate
User friendly UI for easy setup
5 programmable mapping sets with full color LED indication
35 macro keys, up to 1600 actions recordable
Build-in 64Kb onboard memory, plug and play while switching to different PC
Ergonomic design
Adjustable full color LED control
Gold-plated USB connector with braided cable for ensure low latency
Compatible with Windows XP/Vista/7/8
Operating System |
The software supports the following operating systems:
| Windows XP 32 bits
| Windows XP 64 bits
| Windows Vista 32 bits
| Windows Vista 64 bits
| Windows 7 32 bits
| Windows 7 64 bits
| Windows 8 32 bits
| Windows 8 64 bits
Installation |
Step 1 | Plug in TESORO GUNGNIR™ into USB port of your computer
Step 2 | Insert the installation CD into optical drive
Step 3 | Click on the “setup.exe” the setup instruction will guide you through the setup process. Follow the on screen instruction to finish the setup
Step 4 | After successful installation TESORO icon will be displayed on the lower right taskbar
| To get more help or profile macro keys setup for TESORO GUNGNIR™, please run the application program and click
| at the top right-hand corner, or visit TESORO GUNGNIR™ product pages at www.tesorotec.com
Registering your TESORO GUNGNIR™
Visit www.tesorotec.com for online product registration:
One year limited manufacture warranty
Free online technical support
Instruction |
| Software Overview |
|  | Profile:Profile management |  |  | Apply: Save setting and continue
|  | Button Assignment: scroll menu bar to assign button function |  |  | Cancel: Cancel setting and go back to previous status
|  | Advanced Setting: DPI and Macro setting |  |  | OK: Save settings and exit
|  | Mouse Wheel Options: Scroll menu bar to assign function |  |  | About TESORO GUNGNIR™
|  | Mapping: Five mappings for editing and loading profiles |  |  | Close the window
|  | Reset: Reset to default |  |  |
Button Assignment Illustration | Mouse Wheel Setting Illustration
|  | Macro | Load configuration Macro up to the driven menu
|  | Single | Define how to activate function of any single key function configuration
|  | Launch | Define how to open any single program launch
|  | Mapping Switch | Define how to switch different mappings. (+ Scroll Up / + Scroll Down)
Macro Function Configuration 1
|  | Edit New Macro Name |  |  | Macro Status Options:
|  | Macro Record Options: |  |  | Select "save as", "cancel" or "OK.
|  | Select "Start Record" to begin recording; select "Stop Record" |  |  | Macro keys editing window area
|  | to finish recording |  |  |
|  | Setting time delay for specific key: |  |  | List of Macro:
|  | (1) Set selected time delay --> delay time to certain timing (50ms~12750ms) |  |  | Move to specific macro, right click mouse
|  | (2) Set all item delay time to 25ms |  |  | button to edit, rename, or delete
|  | Setting Macro Repeat type: |  |  | Macro:
|  | (1) Repeat-times |  |  | Create new macro or load existing macro
|  | (2) Repeat while pressed |  |  |
|  | (3) Repeat until next key is pressed |  |  |
Macro Function Configuration 2
|  | Colors Setting: |  |  | Speed Setting:
|  | (1) Five colors Mapping files can be defined individually |  |  | Click on the logo to view current speed setting
|  | (2) Activate lighting effect or dimming effect |  |  |
|  | DPI Setting: |  |  | Polling Rate Mapping:
|  | DPI Setting: level one to level four setting |  |  | Four levels polling rate selection: 125HZ, 250HZ, 500HZ and
|  |  |  |  | 1000HZ
After you finish all keys' setting. Click Click to save current profile and continue to set other profiles.
Wait and finish Macro Setting
After click , now you've completed the macro setting, enjoy and have fun ! |