Properties
On the [Properties] tab, you can view and set the properties of the printer.

[Description]
Displays the product name and serial number of the printer. It also allows you to configure the printer name, location, contact person, and administrator's e-mail address.
[Configuration]
Displays the printer specifications, page description languages (PDLs), and memory settings.
[Usage Counters]
Displays the total number of output pages.
[Initialization]
Allows you to initialize NVM and reboot the printer.
[E-mail Alert]
Allows you to configure the settings for the E-mail Alert feature.
[Administrator Security Settings]
Allows you to configure the settings for Administrator Security Settings.
[Port Status]
Allows you to enable or disable each port.
Port Settings:

[Ethernet]
Allows you to configure the settings for Ethernet.

Protocol Settings:

[TCP/IP], [LPD], [Port9100], [FTP], [SNMP], [E-mail], [HTTP]
Allows you to configure the settings for each protocol.
Some items may not appear unless you reboot the printer after selecting [Enabled] under [Port Status].

The following describes how to navigate the [Properties] pages.

Navigating the [Properties] Pages
To display the settings:
Procedure

1. Select an item you want to view or configure in the left frame. If the items below each folder are not displayed, click the [+] sign on the left of each folder to reveal the hidden items.
   The settings of the item are displayed in the right frame.

To change the settings:
Procedure

1. Change the settings using the drop-down menus, text boxes, and check boxes.
   The current settings in the drop down menus are indicated with an asterisk (*).
   Some text boxes accept non-alphanumeric characters. However, if you enter non-alphanumeric characters into text boxes, the entire characters may not be saved even if they are displayed in text boxes. For details, refer to Saving Non-alphanumeric Characters.
2. When you are finished with the settings, click the [Apply] button at the bottom of the right frame.
   The new settings are transmitted and applied to the printer.
   Some settings may not become effective unless you reboot the printer from WebAdmin services or manually switch it off and then on after clicking the [Apply] button.
   When changing the settings, the user name and password of the printer's administrator may be requested. Enter the administrator login ID and password specified in [Administrator Security Settings].
   To cancel the new settings, click the [Undo] button.