Protocol Settings - LPD
This page allows you to configure the settings for LPD.

Connection Time-Out
Set the connection time-out period of LPD protocol. If the reception of data stops before receiving the entire data, the LPD connection to the printer will time out after the time period set here. The time-out period can be set between 1 and 1,000 seconds.

IP Filter
Click this when controlling connections from certain IP addresses. When clicked, [IP Filter] page appears.

[Apply] button
[Undo] button