## Hard Disk Management

In this chapter you will find all the information necessary to carry hard disk operations supported by the program.

### Updating MBR

The program enables to overwrite the current bootable code in the MBR (Master Boot Record) by the standard bootstrap code. This can help to repair a corrupted bootable code of a hard disk resulted from a boot virus attack or a malfunction of boot management software.

In order to update MBR of a hard disk you should take the following steps:

1. Select a hard disk on the Disk Map.

2. Select in the Main Menu: Hard Disk > Update MBR.

| There are other ways to start up this function, please consult the Interface Overview chapter to know more on the subject.

3. The operation will be performed immediately after confirmation.