Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Use Wi-Fi Direct™ > Configure Your Wi-Fi Direct Network > Step-by-step Guide for Wi-Fi Direct Network Configuration

### Step-by-step Guide for Wi-Fi Direct Network Configuration

Related Models:DocuPrint P265 dw
The following instructions offer five methods for configuring your Fuji Xerox machine in a wireless network environment. Select the method you prefer for your environment.

Check your mobile device for configuration.

1. Does your mobile device support Wi-Fi Direct?

   Option | Description
   Yes | Go to Step 2
   No | Go to Step 3

2. Does your mobile device support one-push configuration for Wi-Fi Direct?

   Option | Description
   Yes | See Related Information: Configure Your Wi-Fi Direct Network Using the One-Push Method
   No | See Related Information: Configure Your Wi-Fi Direct Network Using the PIN Method

3. Does your mobile device support Wi-Fi Protected Setup™ (WPS)?

   Option | Description
   Yes | Go to Step 4
   No | See Related Information: Configure Your Wi-Fi Direct Network Manually

4. Does your mobile device support one-push configuration for Wi-Fi Protected Setup™ (WPS)?

   Option | Description
   Yes | See Related Information: Configure Your Wi-Fi Direct Network Using the One-Push Method and Wi-Fi Protected Setup™ (WPS)
   No | See Related Information: Configure Your Wi-Fi Direct Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

To use Fuji Xerox Printer & Scan Utility functionality in a Wi-Fi Direct network configured by one-push configuration using Wi-Fi Direct or by PIN Method configuration using Wi-Fi Direct, the device you use to configure Wi-Fi Direct must be running Android™ 4.0 or greater.

Related Information
  - Configure Your Wi-Fi Direct Network
  - Configure Your Wi-Fi Direct Network Using the One-Push Method
  - Configure Your Wi-Fi Direct Network Using the One-Push Method of Wi-Fi Protected Setup™ (WPS)
  - Configure Your Wi-Fi Direct Network Using the PIN Method
  - Configure Your Wi-Fi Direct Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  - Configure Your Wi-Fi Direct Network Manually

Go to top of page