Home > Routine Maintenance > Replace Supplies

### Replace Supplies

You must replace supplies when the machine indicates that the life of the supply is over.

You can replace the following supplies yourself.

Using non-Fuji Xerox supplies may affect the print quality, hardware performance, and machine reliability.

The toner cartridge and drum unit are two separate supplies. Make sure both are installed as an assembly.

This table lists the indications provide advanced warnings to replace supplies before they reach their end of life. To avoid any inconvenience, you may want to buy spare supplies to keep as replacements before the machine stops printing.

Indication | Supply to get ready | Model name | Approximate life
--- | --- | --- | ---
Toner Low | Toner cartridge | CT202329 *1 CT202330 *2 | 1,200 pages *1 *3 *4 2,600 pages *2 *3 *4
Replace Toner
Toner Ended
Drum ! | Drum unit | CT351055 | 12,000 pages *3 *5
Drum End Soon
Replace Drum

*1
Standard toner cartridge
*2
High yield toner cartridge
*3
A4 or Letter size single-sided pages.
*4
Approximate cartridge yield is declared in accordance with ISO/IEC 19752.
*5
Drum life is approximate and may vary by type of use.

WARNING
  - Never use a vacuum cleaner for spilled toner and residual toner in this product, toner cartridge or toner bottle. It may catch fire by electric sparks inside a vacuum cleaner and cause explosion. Use a broom or a wet cloth to wipe off the spills. If you spill a large volume of toner, contact your local Fuji Xerox representative.
  - Never throw a toner cartridge into an open flame. Remaining toner in the cartridge may catch fire and cause burn injuries or explosion. If you have a used toner cartridge no longer needed, contact your local Fuji Xerox representative for its disposal.

CAUTION
  - Keep drum cartridges (or drum if not a cartridge type) and toner cartridges out of the reach of children. If a child accidentally swallows toner, spit it out, rinse mouth with water, drink water and consult a physician immediately.
  - When replacing drum cartridges (or drum if not a cartridge type) and toner cartridges, be careful not to spill the toner. In case of any toner spills, avoid contact with clothes, skin, eyes and mouth as well as inhalation.
  - If toner spills onto your skin or clothing, wash it off with soap and water. If you get toner particles in the eyes, wash it out with plenty of water for at least 15 minutes until irritation is gone. Consult a physician if necessary.

IMPORTANT
  - Fuji Xerox machines are designed to work with toner of a particular specification and will work to a level of optimum performance when used with Fuji Xerox Original toner cartridges. Fuji Xerox cannot guarantee this optimum performance if toner or toner cartridges of other specifications are used. The machine may not detect toner or toner cartridges of other specifications correctly but may instead detect such items as standard yield toner cartridges. Fuji Xerox does not therefore recommend the use of cartridges other than Fuji Xerox Original cartridges with this machine, or the refilling of empty cartridges with toner from other sources. If damage is caused to the drum unit or other parts of this machine as a result of the use of toner or toner cartridges other than Fuji Xerox Original products due to the incompatibility or lack of suitability of those products with this machine, any repairs required as a result may not be covered by the warranty.
  - For best performance, use a Fuji Xerox Original drum and toner cartridge. Printing with a third party drum unit or toner cartridge may reduce not only the print quality but also the quality and life of the machine itself. Warranty coverage may not apply to problems caused by the use of a third party drum or toner cartridge.

NOTE
  - Availability of toner cartridges differs from one country to another. Contact your local Fuji Xerox office for further details.
  - Be sure to seal up the used supplies tightly in a bag so that toner powder does not spill out of the cartridge.
  - We recommend placing used supplies on a piece of paper to prevent accidentally spilling or scattering the material inside.
  - If you use paper that is not a direct equivalent for the recommended print media, the life of supplies and machine parts may be reduced.
  - The projected life for each of the toner cartridges is based on ISO/IEC 19752. Frequency of replacement will vary depending on the print volume, percentage of coverage, types of media used, and powering on/off the machine.
  - Frequency of replacement supplies except toner cartridges will vary depending on the print volume, types of media used, and powering on/off the machine.
  - Handle the toner cartridge carefully. If toner scatters on your hands or clothes, immediately wipe or wash it off with cold water.
  - To avoid print quality problems, DO NOT touch the shaded parts shown in the illustrations.

    <Toner cartridge>

    <Drum unit>

Related Information
  - Routine Maintenance
  - Learn About The Toner Cartridge
  - Replace the Toner Cartridge
  - Learn About The Drum Unit
  - Replace the Drum Unit
  - Error and Maintenance Messages
  - Error and Maintenance Indications

Go to top of page