Certificate

Overview
  This page allows you to configure a certificate and the corresponding secret key for this print server.
  This print server supports two certification methods. A self-signed certificate and a certificate that is issued by a CA (Certificate Authority).
Use self-signed certificate
  This print server issues its own certificate.
  It is easier to use this type of certificate with functions rather than using a certificate from a CA.
Use a certificate from a CA.
  There are two ways to create a certificate from a CA. Method 1: using a CSR (Certificate Signing Request) from this print server. Method 2: The CA to create a certificate and a secret key.
  Please use this if you already have a CA or would like to use a certificate from an outside trusted CA.
  NOTE:
  Some functions are disabled depending on the status of the certificate configuration.
  The functions are grayed and unlinked.
Certificate List
  Display the list of certificates which are installed on this print server
View
  The contents of the certificate are displayed.
Delete
  Delete the certificate and secret key from this print server
Export
  This print server exports the certificate and secret key.
Create Self-Signed Certificate
  This print server creates a self-signed certificate and installs it by itself.
  It is easier to use this type of certificate with functions rather then using a certificate from a CA.
  There are now two choices to select with the Public Key Algorithim and Digest Algorithim.
  The higher security settings are selected by the default (Public Key Algorithm: RSA2048bit and Digest Algorithm:SHA256).
  When you connect to a device which does not support the higher security, please lower the security settings .
Create CSR
  This print server creates a CSR to be issued with a certificate from a CA.
  After the CA issues a certificate, install the certificate in the page "Install Certificate."
  You can select a Public Key Algorithm and Digest Algorithm security levels, to create a Self-Signed Certificate.
Install Certificate
  This print server installs a certificate from the CA.
  Only a certificate issued with this print server CSR can be installed.
  To use SSL/TLS communication with this print server, the certificate from the CA needs to be installed at the computer communicating with the print server.
  NOTE:
  This function is enabled after creating a CSR.
Import Certificate and Private Key
  This print server imports the certificate and Private key.