## Features of your new product

Your new machine is equipped with a number of special features that improve the quality of the documents you print.

## Special Features

### Print with excellent quality and speed

- You can print with a resolution of up to 1200 x 1200 dpi effective output.

- Your machine prints A4-sized paper at up to 22 ppm and letter-sized paper at up to 23 ppm.

### Handle many different types of printable material

- Manual tray supports plain paper in various sizes, letterhead, envelopes, labels, custom-sized media, postcards, and heavy paper.

- The 250-sheet tray supports plain paper.

### Create professional documents

- Print Watermarks. You can customize your documents with words, such as “Confidential” (See Using watermarks).

- Print Posters. The text and pictures of each page of your document are magnified and printed across the sheet of paper and can then be taped together to form a poster (See Printing posters).

- You can use preprinted forms with plain paper (SeeUsing overlay).

### Save time and money

- To save paper, you can print multiple pages on one single sheet of paper (See Printing multiple pages on one sheet of paper).

- This machine automatically conserves electricity by substantially reducing power consumption when not in use.

- To save paper, you can print on both sides of the paper (manual) (See Printing on both sides of paper (Manual)).

### Print in various environments

- You can print with various operating system such as Windows, Linux and Macintosh systems (See System requirements).

### Copy originals in several formats

- Your machine can copy multiple image copies from the original document on a single page (See 2-up or 4-up copying (N-up)).

- The print quality and image size may be adjusted and enhance at the same time.

### Set a specific time to transmit a Fax

- You can specify a certain time to transmit the fax and also send the fax to several stored destinations.

- After the transmission, the machine may print out the fax reports according to the setting.