Lenovo Digital MFC

This product has the following restrictions and issues.  Please be sure to read this before using.

--------------------------------------------------------------------------------
Installation
--------------------------------------------------------------------------------

When you use Windows Server 2008, install Desktop Experience via Administrative Tools in advance.
(1) Start > Administrative Tools > Server Manager
(2) Click [Add Features].
(3) Select the [Desktop Experience] checkbox and click the [Next] button.
(4) Click the [Install] button.
(5) When installation results are displayed, click the [Close] button.
(6) When you are asked if you want to restart your computer, click the [Yes] button to restart.

--------------------------------------------------------------------------------
M9530				Version 4.22.22.0
--------------------------------------------------------------------------------

This software supports the following models:
- M9530

Issues 
========

1. Notes on Using the WIA Driver
(1) Touch Panel during WIA Connection
- During WIA scan, the operation panel only displays special screens for RemoteScan.
- By pressing the [CANCEL] button on the operation panel, a WIA connection session can be forcibly terminated.
* Buttons other than [CANCEL] are disabled.
* Canceling from the client application or a Network Management Tool scan job is possible.
* WIA scan connection continues until image transfer to the client PC is finished.  Therefore, it may take several minutes before other operations become available after the scan is completed.
(2) Restrictions on the WIA Driver
- No notification report is transmitted whether WIA scan is completed normally or abnormally.
- When power failure occurs during WIA scan, the job will be lost.  Start all over again.

(3) When using Windows Server 2008, set the startup type for the Windows Image Acquisition (WIA) service to [Automatic] using the management tool beforehand.
 1. Right-click [My Computer].
 2. Select [Manage].
 3. Click [Services and Applications].
 4. Click [Services].
 5. Double-click [Windows Image Acquisition (WIA)].
 6. On the [General] tab, select [Automatic] in the [Startup Type] box.
 7. Click [Apply] and [OK].

(4) When using Windows Server 2008, set the startup type for the PnP-X IP Bus Enumerator service to [Automatic] using the management tool beforehand.
 1. Right-click [My Computer].
 2. Select [Manage].
 3. Click [Services and Applications].
 4. Click [Services].
 5. Double-click [PnP-X IP Bus Enumerator].
 6. On the [General] tab, select [Automatic] in the [Startup Type] box.
 7. Click [Apply] and [OK].

(5) When you use an imaging application to scan a document, configure the following settings before scanning:  When the settings have not been configured, scanned images become black.
 1. Select [Tools] -> [Options] -> [Scan] from the imaging application menu bar.
 2. Click the [Advanced] button.
 3. Check [Native].

(6) When you click the [Cancel] button to cancel scanning of a document using Photoshop or other TWAIN-compliant imaging applications, restart the application to scan the document.

(7) Scanning with resolution lower than the default of the scan profile which was set by the client computer may not be performed.
    In that case, set the default resolution of the scan profile to resolution appropriate for scanning.

(8) When the user authentication and department management functions are enabled, a WIA driver cannot be operated from a computer.
    To operate it, disable these functions.

(9) If you use the M9530 MFC on which the user authentication is effective, perform the following procedure before scanning.
 When you use Devices and Printers or Windows Fax and Scan:
 1. In the [New Scan] window, click the [Change] button.
 2. When [Select Device] is displayed, choose the Lenovo Digital MFC and click [Properties] button.
 3. When the department authentication is enabled in the Lenovo Digital MFC, click [Device Settings] tab.
    In another case of authentication, close the Properties dialog box.
 4. Click the [Department Code] button in the Department Code box.
 5. When the User Authentication dialog box is displayed, input the correct department code and click the [OK] button.

When the driver is used from another application, configure similar settings in the Properties dialog box.

--------------------------------------------------------------------------------
Trademarks
--------------------------------------------------------------------------------

- The official name of Windows Vista is Microsoft Windows Vista Operating System.
- The official name of Windows Server 2008 is Microsoft Windows Server 2008 Operating System.
- Microsoft, Windows and the brand names and product names of other Microsoft products are trademarks of Microsoft Corporation in the US and other countries.
- Other company names and product names in this manual are the trademarks of their respective companies.





			December 02, 2011