9. Product Specifications

9.1. Overview

Memory | 128M
Interface Type | USB2.0 and 10/100 Ethernet on certain models
Applicable Platform | Microsoft Windows Server2003/Server2008/Server2012/XP/Vista/Win7/Win8/Win8.1/Win10（32bit&64bit） Mac OS X 10.6/10.7/10.8/10.9
Power Supply | 220V Model: AC 220-240V, 50/60Hz, 4.0A 100V Model: AC 100-127V, 50/60Hz, 8.0A (Note: For the power supply and voltage which are suitable for this printer, please refer to the nameplate at the back of the printer.)
Power Consumption | Printing | 495W Max. Power 750W (25°C)
Standby | 50W
Sleep | 2.0W
Noise | Printing | < 55dB
Standby | < 30dB
Sleep Mode Setting | 1 minute by default
Operation Environment | Operation temperature range (best print quality): 5-35 (10-32)°C Operation humidity range: 20~80% RH
Product Size (W*D*H) mm | 370*370*270mm
Weight (Excluding Laser Cartridge) | About 9kg
Network Capabilities | Protocol Cluster | TCP/IP (IPv4)
Printing Methods | Direct IP (port 9100), LPR/LPD
Management Protocols | DHCP ,SNMPv1, DNS, HTTP
Embedded Web Server Functionality | Configuration/Status via Embedded Web Server
Configuration & Other Services | E-mail Alerts, TCP/IP port access control, Configuration Password, Restore Factory Settings
Application Services | Ping
Addressing | IPv4 32-bit addresses Supports MIB-2, host resources MIB, printer MIB, enterprise MIB Function supported in Internet Explorer 6.0 (or later), Apple Safari 4.0 (or later), MozillaFireFox, Google Chrome, Opera.

9.2. Printing Specification

Print Speed (PPM) | 30/33 (A4) 32/35 (Letter)
Print Language | PCL/PS
Time to First Page | ≤ 8.5s
Maximum print size | Legal (216*355.6mm)
Automatic Duplex | Supported
Paper Input Capacity | Multipurpose Tray | 1 sheet (60~200g/m²)
Standard Tray | 250 sheets (80g/m²)
Paper Output Capacity | Print-side down | 150 sheets (80g/m²)
Print Media | Media Type | Plain, thick, special paper (Transparency, cardstock, label, envelope)
Media Size | A4, A5, JIS B5, IS0 B5, A6, Letter, Legal, Executive, Folio, Oficio, Statement, Japanese Postcard, Monarch Env, DL Env, C5 Env, C6 Env, No.10 Env, ZL, Big 16K, Big 32K, 16K, 32K, B6
Media Weight | 60~200g/m²