// reverb file header and name
[Dee 2.2 Reverb]
name=club

// center frequency of bandpass filter used in reverb
// (float, freq for 44000Hz samplerate)
bandpass_freq=100.0

// Q (width=freq/q) of bandpass filter used in reverb
// Q=0 - filter disabled
bandpass_q=1.0

lDelay[0]=1617
rDelay[0]=1640
lDelay[1]=1116
rDelay[1]=1129
lDelay[2]=1188
rDelay[2]=1211
lDelay[3]=1277
rDelay[3]=1300
lDelay[4]=1356
rDelay[4]=1379
lDelay[5]=1422
rDelay[5]=1455
lDelay[6]=1491
rDelay[6]=1514
lDelay[7]=1557
rDelay[7]=1580

lAllpass[0]=225
rAllpass[0]=249
lAllpass[1]=556
rAllpass[1]=579
lAllpass[2]=441
rAllpass[2]=464
lAllpass[3]=341
rAllpass[3]=364

lAmpDryLeft=0.6
lAmpWetLeft=0.8
lAmpDryRight=0
lAmpWetRight=-0.2
rAmpDryLeft=0
rAmpWetLeft=-0.2
rAmpDryRight=0.6
rAmpWetRight=0.8

ReverbSize=0.5