
          DigitalChina DCN-530TX Fast Ethernet Adapter
                 Windows Me Driver Installation

  Contents:
  ---------
   (A) Installing the driver on Microsoft Windows Me
   (B) Configuring the driver on Microsoft Windows Me

(A) Installing the driver on Microsoft Windows Me
================================================================
    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn on the power, then boot into Windows Me.
    4. Windows Me will find the new hardware automatically,
       then "Add New Hardware Wizard" dialog box will appear.
    5. Select "Specify the location of driver (Advanced)", then
       click "Next" button.
    6. Insert the Driver Diskette.
    7. Select "Search for the best driver for your device.
       (Recommended)." and "Specify a location:". Then type
       "X:\WINME" in the text box. 

      Notice: X: means the floppy drive containing the driver,
      such as: A:, or B: etc.
       
    8. Insert the Driver Diskette and click "Next" button.
    9. Windows Me will find the best driver and prompt with
       "DigitalChina DCN-530TX Fast Ethernet Adapter" in the
       dialog box.
    10. Click "Next" button then Windows Me will copy the driver
       to its system directory.
   11. When Windows prompts with "DigitalChina DCN-530TX Fast
       Ethernet Adapter" in the dialog box, remove the Driver
       Diskette and click the "Finsh" button.
   12. Restart your computer to initialize the network function.

(B) Configuring the driver on Microsoft Windows Me
================================================================

    1. Double Click "My Computer" icon.
    2. Double Click "Control Panel" icon.
    3. Double Click the "Network" icon.
    4. Select the "DigitalChina DCN-530TX Fast Ethernet Adapter"
       from the "Network" dialog box, then click the "Properties"
       button.
    5. Click "Advanced" tab.
    6. There are 5 items in the "Property" box.

       ------Media Type      
       .Specify the media type for the adapter.
       .Default: AutoSense
       
       ------Link Wakeup(Off->On)
       .Specify if Wake on the detection of physical link on is
        enabled.
       .Default: Enabled
       
       ------Link Wakeup(On->Off)
       .Specify if Wake on the detection of physical link off is
        enabled.
       .Default: Disabled

       ------Magic Packet Wakeup
       .Specify if Wake on receiving Magic Packet is enabled.
       .Default: Enabled

       ------Flow Control
       .Specify if 802.3x feature is enabled.
       .Default: Enabled
       
    7. Click "OK" button to return to "Network" dialog box.
    8. Click "OK" button and restart your PC to make the new
       configuration take effect.

Trademarks:
Microsoft Windows Me is a trademark of Microsoft Corporation.
